# datalog_vi key is missing in the Datalogging section of the C:\SPICE\Instrument_CG2_test\Instrument\instrument.ini file.The following error messages were obtained while restoring the experiment status:

The specified default counting channel, , is not a valid counter channel.


5:10:37 PM  2/19/2019    Executing "let __active_table_scans.in_progress "0""

Setting variable "__active_table_scans.in_progress" (current value = "") to "0.000000".

Abort issued!!
# 2/19/2019 5:13:52 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 01.06.
# 2/19/2019 5:13:57 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 01.14.
# 2/19/2019 5:13:58 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 02.11.
# 2/19/2019 5:13:58 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 02.21.
# 2/19/2019 5:13:59 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 03.32.
# 2/19/2019 5:13:59 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 03.36.
# 2/19/2019 5:13:59 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 04.13.
# 2/19/2019 5:13:59 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 04.14.
# 2/19/2019 5:14:00 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 05.06.
# 2/19/2019 5:14:00 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 05.07.
# 2/19/2019 5:14:00 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 05.08.
# 2/19/2019 5:14:00 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 05.09.
# 2/19/2019 5:14:01 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 05.10.
# 2/19/2019 5:14:01 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 05.11.
# 2/19/2019 5:14:01 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 05.18.
# 2/19/2019 5:14:01 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 06.30.
# 2/19/2019 5:14:02 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 07.15.
# 2/19/2019 5:14:02 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 08.25.
# 2/19/2019 5:14:02 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 08.26.
# 2/19/2019 5:14:06 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 11.01.
# 2/19/2019 5:14:06 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 11.02.
# 2/19/2019 5:14:06 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 11.03.
# 2/19/2019 5:14:07 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 11.04.
# 2/19/2019 5:14:07 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 11.05.
# 2/19/2019 5:14:07 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 11.06.
# 2/19/2019 5:14:07 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 11.07.
#  galil_motor_controller_1:  "galil_progs_filename" not found in configuration file
No program file will be loaded.#  galil_motor_controller_2:  "galil_progs_filename" not found in configuration file
No program file will be loaded.#  galil_motor_controller_3:  "galil_progs_filename" not found in configuration file
No program file will be loaded.#  galil_motor_controller_4:  "galil_progs_filename" not found in configuration file
No program file will be loaded.#  galil_motor_controller_6:  "galil_progs_filename" not found in configuration file
No program file will be loaded.#  galil_motor_controller_tilt:  "galil_progs_filename" not found in configuration file
No program file will be loaded.
Motor consistancy check failed for attenuator_pos.
The previously recorded position was 52.99710.
The current position read from the controller is 0.00000.
****Motor [attenuator_pos] initialized to previosly recorded position [52.99710].

***Warning: Motor[beam_trap_x] is below the lower user limit!! (position = 0.000000, lower user limit = 0.200000).
# 
***Warning: Motor[beam_trap_x] is below the lower user limit!! (position = 0.000000, lower user limit = 0.200000).

***Warning: Motor[coll_1] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).
# 
***Warning: Motor[coll_1] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).

***Warning: Motor[coll_2] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).
# 
***Warning: Motor[coll_2] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).

***Warning: Motor[coll_3] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).
# 
***Warning: Motor[coll_3] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).

***Warning: Motor[coll_4] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).
# 
***Warning: Motor[coll_4] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).

***Warning: Motor[coll_5] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).
# 
***Warning: Motor[coll_5] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).

***Warning: Motor[coll_6] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).
# 
***Warning: Motor[coll_6] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).

***Warning: Motor[coll_7] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).
# 
***Warning: Motor[coll_7] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).

***Warning: Motor[coll_8] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).
# 
***Warning: Motor[coll_8] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).

***Warning: Motor[dcal] is below the lower user limit!! (position = 0.000000, lower user limit = 4.900000).
# 
***Warning: Motor[dcal] is below the lower user limit!! (position = 0.000000, lower user limit = 4.900000).

***Warning: Motor[detector_trans] is below the lower user limit!! (position = 0.000000, lower user limit = 0.200000).
# 
***Warning: Motor[detector_trans] is below the lower user limit!! (position = 0.000000, lower user limit = 0.200000).

Motor consistancy check failed for flange_det_dist.
The previously recorded position was 2.37000.
The current position read from the controller is 0.74900.
****Motor [flange_det_dist] initialized to previosly recorded position [2.37000].

Motor consistancy check failed for sample_x.
The previously recorded position was 176.69817.
The current position read from the controller is 0.00000.
****Motor [sample_x] initialized to previosly recorded position [176.69817].

***Warning: Motor[trap_y_101mm] is below the lower user limit!! (position = -0.000049, lower user limit = 0.000000).
# 
***Warning: Motor[trap_y_101mm] is below the lower user limit!! (position = -0.000049, lower user limit = 0.000000).

Motor consistancy check failed for trap_y_25mm.
The previously recorded position was 1.00005.
The current position read from the controller is 0.00000.
****Motor [trap_y_25mm] initialized to previosly recorded position [1.00005].

Motor consistancy check failed for trap_y_50mm.
The previously recorded position was 1.00005.
The current position read from the controller is 0.00000.
****Motor [trap_y_50mm] initialized to previosly recorded position [1.00005].

Motor consistancy check failed for trap_y_76mm.
The previously recorded position was 1.00005.
The current position read from the controller is 0.00000.
****Motor [trap_y_76mm] initialized to previosly recorded position [1.00005].
The following error messages were obtained while restoring the experiment status:

The specified default counting channel, , is not a valid counter channel.

# 2/19/2019 5:15:03 PM	At GP-SANS the PLC has registered a Vacuum Alarm.

5:15:06 PM  2/19/2019    Executing "let __active_table_scans.in_progress "0""

Setting variable "__active_table_scans.in_progress" (current value = "") to "0.000000".

Abort issued!!
# 2/19/2019 5:53:35 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 01.06.
# 2/19/2019 5:53:35 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 01.14.
# 2/19/2019 5:53:36 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 02.11.
# 2/19/2019 5:53:36 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 02.21.
# 2/19/2019 5:53:36 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 03.32.
# 2/19/2019 5:53:36 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 03.36.
# 2/19/2019 5:53:37 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 04.13.
# 2/19/2019 5:53:37 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 04.14.
# 2/19/2019 5:53:37 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 05.06.
# 2/19/2019 5:53:37 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 05.07.
# 2/19/2019 5:53:38 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 05.08.
# 2/19/2019 5:53:42 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 05.09.
# 2/19/2019 5:53:42 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 05.10.
# 2/19/2019 5:53:42 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 05.11.
# 2/19/2019 5:53:42 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 05.18.
# 2/19/2019 5:53:43 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 06.30.
# 2/19/2019 5:53:43 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 07.15.
# 2/19/2019 5:53:51 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 08.25.
# 2/19/2019 5:53:52 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 08.26.
# 2/19/2019 5:53:59 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 11.01.
# 2/19/2019 5:53:59 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 11.02.
# 2/19/2019 5:54:00 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 11.03.
# 2/19/2019 5:54:00 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 11.04.
# 2/19/2019 5:54:00 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 11.05.
# 2/19/2019 5:54:00 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 11.06.
# 2/19/2019 5:54:01 PM:  Fault communicating with the device:  . UniDrive did not accept change in parameter 11.07.
#  galil_motor_controller_1:  "galil_progs_filename" not found in configuration file
No program file will be loaded.#  galil_motor_controller_2:  "galil_progs_filename" not found in configuration file
No program file will be loaded.#  galil_motor_controller_3:  "galil_progs_filename" not found in configuration file
No program file will be loaded.#  galil_motor_controller_4:  "galil_progs_filename" not found in configuration file
No program file will be loaded.#  galil_motor_controller_6:  "galil_progs_filename" not found in configuration file
No program file will be loaded.#  galil_motor_controller_tilt:  "galil_progs_filename" not found in configuration file
No program file will be loaded.
Motor consistancy check failed for attenuator_pos.
The previously recorded position was 52.99710.
The current position read from the controller is 0.00000.
****Motor [attenuator_pos] initialized to previosly recorded position [52.99710].

***Warning: Motor[beam_trap_x] is below the lower user limit!! (position = 0.000000, lower user limit = 0.200000).
# 
***Warning: Motor[beam_trap_x] is below the lower user limit!! (position = 0.000000, lower user limit = 0.200000).

***Warning: Motor[coll_1] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).
# 
***Warning: Motor[coll_1] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).

***Warning: Motor[coll_2] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).
# 
***Warning: Motor[coll_2] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).

***Warning: Motor[coll_3] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).
# 
***Warning: Motor[coll_3] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).

***Warning: Motor[coll_4] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).
# 
***Warning: Motor[coll_4] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).

***Warning: Motor[coll_5] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).
# 
***Warning: Motor[coll_5] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).

***Warning: Motor[coll_6] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).
# 
***Warning: Motor[coll_6] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).

***Warning: Motor[coll_7] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).
# 
***Warning: Motor[coll_7] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).

***Warning: Motor[coll_8] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).
# 
***Warning: Motor[coll_8] is below the lower user limit!! (position = 0.000000, lower user limit = 0.100000).

***Warning: Motor[dcal] is below the lower user limit!! (position = 0.000000, lower user limit = 4.900000).
# 
***Warning: Motor[dcal] is below the lower user limit!! (position = 0.000000, lower user limit = 4.900000).

***Warning: Motor[detector_trans] is below the lower user limit!! (position = 0.000000, lower user limit = 0.200000).
# 
***Warning: Motor[detector_trans] is below the lower user limit!! (position = 0.000000, lower user limit = 0.200000).

Motor consistancy check failed for flange_det_dist.
The previously recorded position was 2.37000.
The current position read from the controller is 0.74900.
****Motor [flange_det_dist] initialized to previosly recorded position [2.37000].

Motor consistancy check failed for sample_x.
The previously recorded position was 176.69817.
The current position read from the controller is 0.00000.
****Motor [sample_x] initialized to previosly recorded position [176.69817].

***Warning: Motor[trap_y_101mm] is below the lower user limit!! (position = -0.000049, lower user limit = 0.000000).
# 
***Warning: Motor[trap_y_101mm] is below the lower user limit!! (position = -0.000049, lower user limit = 0.000000).

Motor consistancy check failed for trap_y_25mm.
The previously recorded position was 1.00005.
The current position read from the controller is 0.00000.
****Motor [trap_y_25mm] initialized to previosly recorded position [1.00005].

Motor consistancy check failed for trap_y_50mm.
The previously recorded position was 1.00005.
The current position read from the controller is 0.00000.
****Motor [trap_y_50mm] initialized to previosly recorded position [1.00005].

Motor consistancy check failed for trap_y_76mm.
The previously recorded position was 1.00005.
The current position read from the controller is 0.00000.
****Motor [trap_y_76mm] initialized to previosly recorded position [1.00005].
The following error messages were obtained while restoring the experiment status:

The specified default counting channel, , is not a valid counter channel.

# 2/19/2019 5:54:42 PM	At GP-SANS the PLC has registered a Vacuum Alarm.
# 2/19/2019 5:57:25 PM	The velocity selector at CG2 is indicating there is a fault in the drive controller (5:57:26 PM on 2/19/2019).

5:57:53 PM  2/19/2019    Executing "let __active_table_scans.in_progress "0""

Setting variable "__active_table_scans.in_progress" (current value = "") to "0.000000".

Abort issued!!
# motor_controller not found in configuration file.
no default -- device will be disabled.# Device: vs1  Error: controller not found in the configuration file. No default -- device will be disabled.
 # motor_controller not found in configuration file.
no default -- device will be disabled.# Device: vs_current  Error: controller not found in the configuration file. No default -- device will be disabled.
 # Device: vs_speed_pv  Error: controller not found in the configuration file. No default -- device will be disabled.
 # Device: vs_current  Error: controller not found in the configuration file. No default -- device will be disabled.
 # Device: vs_speed_pv  Error: controller not found in the configuration file. No default -- device will be disabled.
 # Device: vs_current  Error: Fault in parameter method -
 get_motor_position # Device: vs_speed_pv  Error: Fault in parameter method -
 get_motor_position # Device: vs_current  Error: Fault in parameter method -
 get_motor_position # Device: vs_speed_pv  Error: Fault in parameter method -
 get_motor_position The following error messages were obtained while restoring the experiment status:

The specified default counting channel, , is not a valid counter channel.

# Device: vs_current  Error: Fault in parameter method -
 get_motor_position # Device: vs_speed_pv  Error: Fault in parameter method -
 get_motor_position # Device: vs_current  Error: Fault in parameter method -
 get_motor_position # Device: vs_speed_pv  Error: Fault in parameter method -
 get_motor_position # Device: vs_current  Error: Fault in parameter method -
 get_motor_position # Device: vs_speed_pv  Error: Fault in parameter method -
 get_motor_position # Device: vs_current  Error: Fault in parameter method -
 get_motor_position # Device: vs_speed_pv  Error: Fault in parameter method -
 get_motor_position 
9:56:45 AM  2/20/2019    Executing "let __active_table_scans.in_progress "0""

Setting variable "__active_table_scans.in_progress" (current value = "") to "0.000000".

Abort issued!!
The following error messages were obtained while restoring the experiment status:

The specified default counting channel, , is not a valid counter channel.


10:04:10 AM  2/20/2019    Executing "let __active_table_scans.in_progress "0""

Setting variable "__active_table_scans.in_progress" (current value = "") to "0.000000".

Abort issued!!
The following error messages were obtained while restoring the experiment status:

The specified default counting channel, , is not a valid counter channel.

# 2/20/2019 10:06:40 AM	At GP-SANS the PLC has registered a Vacuum Alarm.
# 2/20/2019 10:36:40 AM	At GP-SANS the PLC has registered a Vacuum Alarm.

10:51:38 AM  2/20/2019    Executing "let __active_table_scans.in_progress "0""

Setting variable "__active_table_scans.in_progress" (current value = "") to "0.000000".

Abort issued!!
The following error messages were obtained while restoring the experiment status:

The specified default counting channel, , is not a valid counter channel.

# 2/20/2019 10:52:24 AM	At GP-SANS the PLC has registered a Vacuum Alarm.

10:55:44 AM  2/20/2019    Executing "comment "--------------------Begin Table Scans/Sample Scans Preamble""

COMMENT:
--------------------Begin Table Scans/Sample Scans Preamble


10:55:44 AM  2/20/2019    Executing "reset_active_scan_data"

Resetting active scan data.
10:55:45 AM  2/20/2019    Executing "scantitle """

Setting the scantitle to:



10:55:45 AM  2/20/2019    Executing "set_sample_info_sample_changer "Flat changer" 8"

Setting sample info sample changer name to Flat changer 
with 8 changer positions.

10:55:45 AM  2/20/2019    Executing "set_sample_info_instrument_config "TwoConfigI" "Mid Q,High Q""

Setting sample info instrument configuration name to TwoConfigI.
 
10:55:45 AM  2/20/2019    Executing "set_sample_info_parameter_config "No Parameters" "" """

Setting sample info parameter configuration name to No Parameters.
 
10:55:45 AM  2/20/2019    Executing "set_sample_info_setup_order "Mid Q,High Q""

Setting sample info setup order to "Mid Q,High Q".

10:55:45 AM  2/20/2019    Executing "set_sample_info_scan_order "Setup Order""

Setting sample info scan order to "Setup Order".
 
10:55:46 AM  2/20/2019    Executing "set_sample_info_do_transmission_scans "false""

Setting sample info do_transmission_scans to "false".

10:55:46 AM  2/20/2019    Executing "set_sample_info_specify_frames "false""

Setting sample info specify_frames to "false".
 
10:55:46 AM  2/20/2019    Executing "set_sample_info_background_columns_names "Cell Thickness (mm)""

Setting sample info background columns names to "Cell Thickness (mm)".
 
10:55:46 AM  2/20/2019    Executing "set_sample_info_background_columns_default_values "True""

Setting sample info background columns default values to "True".
 
10:55:46 AM  2/20/2019    Executing "set_sample_info_sample_columns_names """

Setting sample info sample columns names to "".
 
10:55:46 AM  2/20/2019    Executing "set_sample_info_sample_columns_default_values """

Setting sample info sample columns default values to "".
 
10:55:46 AM  2/20/2019    Executing "set_sample_info_sample_id 1 """

Setting sample info sample id to  
for changer position 1.

10:55:46 AM  2/20/2019    Executing "set_sample_info_sample_name 1 "open""

Setting sample info sample name to open 
for changer position 1.

10:55:47 AM  2/20/2019    Executing "set_sample_info_sample_thickness 1 "1.000000""

Setting sample info sample thickness to 1.000000 mm 
for changer position 1.

10:55:47 AM  2/20/2019    Executing "set_sample_info_sample_columns_values 1 ",""

Setting sample info sample columns values to "," 
for changer position 1.

10:55:47 AM  2/20/2019    Executing "set_sample_info_background_columns_values 1 "True""

Setting sample info background columns values to "True" 
for changer position 1.

10:55:47 AM  2/20/2019    Executing "set_sample_info_sample_type 1 "Open Beam""

Setting sample info sample type to Open Beam 
for changer position 1.

10:55:47 AM  2/20/2019    Executing "set_sample_info_do_scan 1 "true""

Setting sample info do_scan value to true 
for changer position 1.

10:55:47 AM  2/20/2019    Executing "set_sample_info_scan_times 1 "2.000000,2.000000""

Setting sample info scan times values to "2.000000,2.000000" 
for changer position 1.

10:55:47 AM  2/20/2019    Executing "set_sample_info_frame_counts 1 "1,1""

Setting sample info frame counts values to "1,1" 
for changer position 1.

10:55:47 AM  2/20/2019    Executing "set_sample_info_parameter_columns_values 1 """

Setting sample info parameter columns values to "" 
for changer position 1.

10:55:47 AM  2/20/2019    Executing "set_sample_info_sample_id 2 """

Setting sample info sample id to  
for changer position 2.

10:55:47 AM  2/20/2019    Executing "set_sample_info_sample_name 2 "H2O""

Setting sample info sample name to H2O 
for changer position 2.

10:55:48 AM  2/20/2019    Executing "set_sample_info_sample_thickness 2 "1.000000""

Setting sample info sample thickness to 1.000000 mm 
for changer position 2.

10:55:48 AM  2/20/2019    Executing "set_sample_info_sample_columns_values 2 """

Setting sample info sample columns values to "" 
for changer position 2.

10:55:48 AM  2/20/2019    Executing "set_sample_info_background_columns_values 2 "True""

Setting sample info background columns values to "True" 
for changer position 2.

10:55:48 AM  2/20/2019    Executing "set_sample_info_sample_type 2 "Sample""

Setting sample info sample type to Sample 
for changer position 2.

10:55:48 AM  2/20/2019    Executing "set_sample_info_do_scan 2 "true""

Setting sample info do_scan value to true 
for changer position 2.

10:55:48 AM  2/20/2019    Executing "set_sample_info_scan_times 2 "2.000000,2.000000""

Setting sample info scan times values to "2.000000,2.000000" 
for changer position 2.

10:55:48 AM  2/20/2019    Executing "set_sample_info_frame_counts 2 "1,1""

Setting sample info frame counts values to "1,1" 
for changer position 2.

10:55:48 AM  2/20/2019    Executing "set_sample_info_parameter_columns_values 2 """

Setting sample info parameter columns values to "" 
for changer position 2.

10:55:48 AM  2/20/2019    Executing "set_sample_info_sample_id 3 """

Setting sample info sample id to  
for changer position 3.

10:55:48 AM  2/20/2019    Executing "set_sample_info_sample_name 3 "AgBeh""

Setting sample info sample name to AgBeh 
for changer position 3.

10:55:49 AM  2/20/2019    Executing "set_sample_info_sample_thickness 3 "1.000000""

Setting sample info sample thickness to 1.000000 mm 
for changer position 3.

10:55:49 AM  2/20/2019    Executing "set_sample_info_sample_columns_values 3 """

Setting sample info sample columns values to "" 
for changer position 3.

10:55:49 AM  2/20/2019    Executing "set_sample_info_background_columns_values 3 "True""

Setting sample info background columns values to "True" 
for changer position 3.

10:55:49 AM  2/20/2019    Executing "set_sample_info_sample_type 3 "Sample""

Setting sample info sample type to Sample 
for changer position 3.

10:55:49 AM  2/20/2019    Executing "set_sample_info_do_scan 3 "false""

Setting sample info do_scan value to false 
for changer position 3.

10:55:49 AM  2/20/2019    Executing "set_sample_info_scan_times 3 "0.000000,300.000000""

Setting sample info scan times values to "0.000000,300.000000" 
for changer position 3.

10:55:50 AM  2/20/2019    Executing "set_sample_info_frame_counts 3 "1,1""

Setting sample info frame counts values to "1,1" 
for changer position 3.

10:55:50 AM  2/20/2019    Executing "set_sample_info_parameter_columns_values 3 """

Setting sample info parameter columns values to "" 
for changer position 3.

10:55:50 AM  2/20/2019    Executing "set_sample_info_sample_id 4 """

Setting sample info sample id to  
for changer position 4.

10:55:50 AM  2/20/2019    Executing "set_sample_info_sample_name 4 "5""

Setting sample info sample name to 5 
for changer position 4.

10:55:50 AM  2/20/2019    Executing "set_sample_info_sample_thickness 4 "1.000000""

Setting sample info sample thickness to 1.000000 mm 
for changer position 4.

10:55:50 AM  2/20/2019    Executing "set_sample_info_sample_columns_values 4 """

Setting sample info sample columns values to "" 
for changer position 4.

10:55:50 AM  2/20/2019    Executing "set_sample_info_background_columns_values 4 "True""

Setting sample info background columns values to "True" 
for changer position 4.

10:55:50 AM  2/20/2019    Executing "set_sample_info_sample_type 4 "Sample""

Setting sample info sample type to Sample 
for changer position 4.

10:55:50 AM  2/20/2019    Executing "set_sample_info_do_scan 4 "false""

Setting sample info do_scan value to false 
for changer position 4.

10:55:50 AM  2/20/2019    Executing "set_sample_info_scan_times 4 "0.000000,300.000000""

Setting sample info scan times values to "0.000000,300.000000" 
for changer position 4.

10:55:51 AM  2/20/2019    Executing "set_sample_info_frame_counts 4 "1,1""

Setting sample info frame counts values to "1,1" 
for changer position 4.

10:55:51 AM  2/20/2019    Executing "set_sample_info_parameter_columns_values 4 """

Setting sample info parameter columns values to "" 
for changer position 4.

10:55:51 AM  2/20/2019    Executing "set_sample_info_sample_id 5 """

Setting sample info sample id to  
for changer position 5.

10:55:51 AM  2/20/2019    Executing "set_sample_info_sample_name 5 """

Setting sample info sample name to  
for changer position 5.

10:55:51 AM  2/20/2019    Executing "set_sample_info_sample_thickness 5 "1.000000""

Setting sample info sample thickness to 1.000000 mm 
for changer position 5.

10:55:51 AM  2/20/2019    Executing "set_sample_info_sample_columns_values 5 """

Setting sample info sample columns values to "" 
for changer position 5.

10:55:51 AM  2/20/2019    Executing "set_sample_info_background_columns_values 5 "True""

Setting sample info background columns values to "True" 
for changer position 5.

10:55:51 AM  2/20/2019    Executing "set_sample_info_sample_type 5 "Sample""

Setting sample info sample type to Sample 
for changer position 5.

10:55:51 AM  2/20/2019    Executing "set_sample_info_do_scan 5 "false""

Setting sample info do_scan value to false 
for changer position 5.

10:55:51 AM  2/20/2019    Executing "set_sample_info_scan_times 5 "0.000000,300.000000""

Setting sample info scan times values to "0.000000,300.000000" 
for changer position 5.

10:55:52 AM  2/20/2019    Executing "set_sample_info_frame_counts 5 "1,1""

Setting sample info frame counts values to "1,1" 
for changer position 5.

10:55:52 AM  2/20/2019    Executing "set_sample_info_parameter_columns_values 5 """

Setting sample info parameter columns values to "" 
for changer position 5.

10:55:52 AM  2/20/2019    Executing "set_sample_info_sample_id 6 """

Setting sample info sample id to  
for changer position 6.

10:55:52 AM  2/20/2019    Executing "set_sample_info_sample_name 6 """

Setting sample info sample name to  
for changer position 6.

10:55:52 AM  2/20/2019    Executing "set_sample_info_sample_thickness 6 "1.000000""

Setting sample info sample thickness to 1.000000 mm 
for changer position 6.

10:55:52 AM  2/20/2019    Executing "set_sample_info_sample_columns_values 6 """

Setting sample info sample columns values to "" 
for changer position 6.

10:55:52 AM  2/20/2019    Executing "set_sample_info_background_columns_values 6 "True""

Setting sample info background columns values to "True" 
for changer position 6.

10:55:52 AM  2/20/2019    Executing "set_sample_info_sample_type 6 "Sample""

Setting sample info sample type to Sample 
for changer position 6.

10:55:52 AM  2/20/2019    Executing "set_sample_info_do_scan 6 "false""

Setting sample info do_scan value to false 
for changer position 6.

10:55:52 AM  2/20/2019    Executing "set_sample_info_scan_times 6 "0.000000,300.000000""

Setting sample info scan times values to "0.000000,300.000000" 
for changer position 6.

10:55:53 AM  2/20/2019    Executing "set_sample_info_frame_counts 6 "1,1""

Setting sample info frame counts values to "1,1" 
for changer position 6.

10:55:53 AM  2/20/2019    Executing "set_sample_info_parameter_columns_values 6 """

Setting sample info parameter columns values to "" 
for changer position 6.

10:55:53 AM  2/20/2019    Executing "set_sample_info_sample_id 7 """

Setting sample info sample id to  
for changer position 7.

10:55:53 AM  2/20/2019    Executing "set_sample_info_sample_name 7 """

Setting sample info sample name to  
for changer position 7.

10:55:53 AM  2/20/2019    Executing "set_sample_info_sample_thickness 7 "1.000000""

Setting sample info sample thickness to 1.000000 mm 
for changer position 7.

10:55:53 AM  2/20/2019    Executing "set_sample_info_sample_columns_values 7 """

Setting sample info sample columns values to "" 
for changer position 7.

10:55:53 AM  2/20/2019    Executing "set_sample_info_background_columns_values 7 "True""

Setting sample info background columns values to "True" 
for changer position 7.

10:55:53 AM  2/20/2019    Executing "set_sample_info_sample_type 7 "Sample""

Setting sample info sample type to Sample 
for changer position 7.

10:55:53 AM  2/20/2019    Executing "set_sample_info_do_scan 7 "false""

Setting sample info do_scan value to false 
for changer position 7.

10:55:53 AM  2/20/2019    Executing "set_sample_info_scan_times 7 "0.000000,300.000000""

Setting sample info scan times values to "0.000000,300.000000" 
for changer position 7.

10:55:54 AM  2/20/2019    Executing "set_sample_info_frame_counts 7 "1,1""

Setting sample info frame counts values to "1,1" 
for changer position 7.

10:55:54 AM  2/20/2019    Executing "set_sample_info_parameter_columns_values 7 """

Setting sample info parameter columns values to "" 
for changer position 7.

10:55:54 AM  2/20/2019    Executing "set_sample_info_sample_id 8 """

Setting sample info sample id to  
for changer position 8.

10:55:54 AM  2/20/2019    Executing "set_sample_info_sample_name 8 "R10_20""

Setting sample info sample name to R10_20 
for changer position 8.

10:55:54 AM  2/20/2019    Executing "set_sample_info_sample_thickness 8 "1.000000""

Setting sample info sample thickness to 1.000000 mm 
for changer position 8.

10:55:54 AM  2/20/2019    Executing "set_sample_info_sample_columns_values 8 """

Setting sample info sample columns values to "" 
for changer position 8.

10:55:54 AM  2/20/2019    Executing "set_sample_info_background_columns_values 8 "True""

Setting sample info background columns values to "True" 
for changer position 8.

10:55:55 AM  2/20/2019    Executing "set_sample_info_sample_type 8 "Sample""

Setting sample info sample type to Sample 
for changer position 8.

10:55:55 AM  2/20/2019    Executing "set_sample_info_do_scan 8 "false""

Setting sample info do_scan value to false 
for changer position 8.

10:55:55 AM  2/20/2019    Executing "set_sample_info_scan_times 8 "0.000000,300.000000""

Setting sample info scan times values to "0.000000,300.000000" 
for changer position 8.

10:55:55 AM  2/20/2019    Executing "set_sample_info_frame_counts 8 "1,1""

Setting sample info frame counts values to "1,1" 
for changer position 8.

10:55:55 AM  2/20/2019    Executing "set_sample_info_parameter_columns_values 8 """

Setting sample info parameter columns values to "" 
for changer position 8.

10:55:55 AM  2/20/2019    Executing "use_sample_changer "Flat changer""

Setting active sample changer to Flat changer.

10:55:55 AM  2/20/2019    Executing "use_instrument_config "TwoConfigI""

Setting active instrument config to TwoConfigI.

10:55:55 AM  2/20/2019    Executing "use_parameter_config "No Parameters""

Setting active parameter config to No Parameters.

10:55:55 AM  2/20/2019    Executing "comment "--------------------End Table Scans/Sample Scans Preamble""

COMMENT:
--------------------End Table Scans/Sample Scans Preamble


10:55:56 AM  2/20/2019    Executing "reset_active_table_scans"

Resetting active table scan command info.
10:55:56 AM  2/20/2019    Executing "set_table_scan_command_info "do_table_scan 1 \22Mid Q\22 \22Scattering\22 1" 1 "open" "Mid Q" "Scattering" 2.000000 1 2.000000"

Setting  info for next table scan command.

10:55:56 AM  2/20/2019    Executing "set_table_scan_command_info "do_table_scan 2 \22Mid Q\22 \22Scattering\22 2" 2 "H2O" "Mid Q" "Scattering" 2.000000 1 2.000000"

Setting  info for next table scan command.

10:55:56 AM  2/20/2019    Executing "set_table_scan_command_info "do_table_scan 1 \22High Q\22 \22Scattering\22 3" 1 "open" "High Q" "Scattering" 2.000000 1 2.000000"

Setting  info for next table scan command.

10:55:56 AM  2/20/2019    Executing "set_table_scan_command_info "do_table_scan 2 \22High Q\22 \22Scattering\22 4" 2 "H2O" "High Q" "Scattering" 2.000000 1 2.000000"

Setting  info for next table scan command.

10:55:56 AM  2/20/2019    Executing "let __active_table_scans.in_progress "1""

Setting variable "__active_table_scans.in_progress" (current value = "0") to "1.000000".

10:55:56 AM  2/20/2019    Executing "do_table_scan 1 "Mid Q" "Scattering" 1"


10:55:56 AM  2/20/2019    Executing "table_scan_initialize 1"

Initializing info for next table scan command.

10:55:56 AM  2/20/2019    Executing "do_table_scan 1 "Mid Q" "Scattering""


10:55:57 AM  2/20/2019    Executing "use_changer_pos 1"

Setting active sample changer position to 1 (valid sample info found).

10:55:57 AM  2/20/2019    Executing "use_setup "Mid Q" "Scattering""

Setting active setup to Mid Q and scan type to Scattering.

10:55:57 AM  2/20/2019    Executing "set_table_scan_title"

Automatically generating
scan title for table scan to:
open(IC: TwoConfigI  S: Mid Q  P:[])


10:55:57 AM  2/20/2019    Executing "do_parameters_start"


10:55:58 AM  2/20/2019    Executing "go_changer_pos"


10:55:58 AM  2/20/2019    Executing "drive sample_x -178.900000"

SPICE Error in drive command: Wed, Feb 20, 2019 [10:55:58 AM] : SPICE Error in Common.lvlib:Common_Commands.lvlib:Drive_Motor_Val_Pairs.vi.

The argument for motor sample_x, "" contains more than one motor position.

..Move aborted.


10:55:58 AM  2/20/2019    Executing "go_setup"


10:55:58 AM  2/20/2019    Executing "go_setup_beam_trap_in"


10:55:58 AM  2/20/2019    Executing "drive dlambda 0.132000"

Driving to the following position: ""

Destination Motor Positions:
motor           position
selector_tilt   -0.01894

Drive completed.


10:56:07 AM  2/20/2019    Executing "drive beam_trap_x 79.000000 trap_y_76mm 552.000000 sdd 8.844000 detector_trans 400.000000 lambda 4.750000"

Driving to the following position: ""

Destination Motor Positions:
motor           position
beam_trap_x     79.00000
trap_y_76mm     552.00000
detector_trans  400.00000
flange_det_dist 8.80000
selector_speed  5652.82678

Drive completed.


10:56:24 AM  2/20/2019    Executing "if @(hv)<0.5 drive hv 1"


10:56:24 AM  2/20/2019    Executing "do_parameters_finish"


10:56:25 AM  2/20/2019    Executing "go_attenuator"


10:56:25 AM  2/20/2019    Executing "drive attenuator_pos open"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -449.00000

Drive completed.


10:56:25 AM  2/20/2019    Executing "table_scan_counting_initialize"

Initializing counting for current table scan command.

10:56:25 AM  2/20/2019    Executing "scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)"


# scan = 1
# date = 2/20/2019
# time = 10:56:25 AM
# experiment = 
# experiment_number = 0
# ipts_number = undefined
# cycle_number = undefined
# command = scan n=@(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# builtin_command = scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# users = 
# local_contact = 
# scan_title = open(IC: TwoConfigI  S: Mid Q  P:[])
# samplename = open
# sampletype = Open Beam
# preset_type = normal 
# preset_channel = time
# preset_value = 2.000000
# def_x = Pt.
# def_y = 
# col_headers = 
#   Pt.       time   detector    monitor selector_speed selector_tilt    nguides attenuator_pos beam_trap_x       dcal detector_trans flange_det_dist         hv trap_y_101mm trap_y_25mm trap_y_50mm trap_y_76mm
      1      2.392   1395.000    538.000  5652.7184    -0.0193     4.0000  -449.0125    79.0008     0.0000   400.0001     8.8029     0.9978     0.9998     0.9980     0.9993   551.997
# Footer Info = Add information here
# 10:56:28 AM  2/20/2019   scan completed.

10:56:28 AM  2/20/2019    Executing "table_scan_counting_finalize"

Finalizing counting for current table scan command.

10:56:28 AM  2/20/2019    Executing "go_attenuator_non_open"


10:56:28 AM  2/20/2019    Executing "drive attenuator_pos x10k"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -130.00000

Drive completed.


10:56:29 AM  2/20/2019    Executing "reset_active_changer_pos_data"

Resetting active changer position data.
10:56:29 AM  2/20/2019    Executing "table_scan_finalize 1"

Finalizing info for next table scan command.

10:56:30 AM  2/20/2019    Executing "do_table_scan 2 "Mid Q" "Scattering" 2"


10:56:30 AM  2/20/2019    Executing "table_scan_initialize 2"

Initializing info for next table scan command.

10:56:30 AM  2/20/2019    Executing "do_table_scan 2 "Mid Q" "Scattering""


10:56:30 AM  2/20/2019    Executing "use_changer_pos 2"

Setting active sample changer position to 2 (valid sample info found).

10:56:30 AM  2/20/2019    Executing "use_setup "Mid Q" "Scattering""

Setting active setup to Mid Q and scan type to Scattering.

10:56:32 AM  2/20/2019    Executing "set_table_scan_title"

Automatically generating
scan title for table scan to:
H2O(IC: TwoConfigI  S: Mid Q  P:[])


10:56:32 AM  2/20/2019    Executing "do_parameters_start"


10:56:32 AM  2/20/2019    Executing "go_changer_pos"


10:56:33 AM  2/20/2019    Executing "drive sample_x -128.100000"

SPICE Error in drive command: Wed, Feb 20, 2019 [10:56:33 AM] : SPICE Error in Common.lvlib:Common_Commands.lvlib:Drive_Motor_Val_Pairs.vi.

The argument for motor sample_x, "" contains more than one motor position.

..Move aborted.


10:56:33 AM  2/20/2019    Executing "go_setup"


10:56:33 AM  2/20/2019    Executing "go_setup_beam_trap_in"


10:56:33 AM  2/20/2019    Executing "drive attenuator_pos x10k"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -130.00000

Drive completed.


10:56:33 AM  2/20/2019    Executing "if @(hv)<0.5 drive hv 1"


10:56:33 AM  2/20/2019    Executing "do_parameters_finish"


10:56:33 AM  2/20/2019    Executing "go_attenuator"


10:56:34 AM  2/20/2019    Executing "drive attenuator_pos open"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -449.00000

Drive completed.


10:56:34 AM  2/20/2019    Executing "table_scan_counting_initialize"

Initializing counting for current table scan command.

10:56:34 AM  2/20/2019    Executing "scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)"


# scan = 2
# date = 2/20/2019
# time = 10:56:34 AM
# experiment = 
# experiment_number = 0
# ipts_number = undefined
# cycle_number = undefined
# command = scan n=@(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# builtin_command = scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# users = 
# local_contact = 
# scan_title = H2O(IC: TwoConfigI  S: Mid Q  P:[])
# samplename = H2O
# sampletype = Sample
# preset_type = normal 
# preset_channel = time
# preset_value = 2.000000
# def_x = Pt.
# def_y = 
# col_headers = 
#   Pt.       time   detector    monitor selector_speed selector_tilt    nguides attenuator_pos beam_trap_x       dcal detector_trans flange_det_dist         hv trap_y_101mm trap_y_25mm trap_y_50mm trap_y_76mm
      1      2.383   1073.000    491.000  5652.7184    -0.0193     4.0000  -449.0192    79.0008     0.0000   400.0001     8.8029     0.9978     0.9998     0.9980     0.9993   551.997
# Footer Info = Add information here
# 10:56:37 AM  2/20/2019   scan completed.

10:56:37 AM  2/20/2019    Executing "table_scan_counting_finalize"

Finalizing counting for current table scan command.

10:56:37 AM  2/20/2019    Executing "go_attenuator_non_open"


10:56:37 AM  2/20/2019    Executing "drive attenuator_pos x10k"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -130.00000

Drive completed.


10:56:38 AM  2/20/2019    Executing "reset_active_changer_pos_data"

Resetting active changer position data.
10:56:38 AM  2/20/2019    Executing "table_scan_finalize 2"

Finalizing info for next table scan command.

10:56:38 AM  2/20/2019    Executing "do_table_scan 1 "High Q" "Scattering" 3"


10:56:38 AM  2/20/2019    Executing "table_scan_initialize 3"

Initializing info for next table scan command.

10:56:38 AM  2/20/2019    Executing "do_table_scan 1 "High Q" "Scattering""


10:56:38 AM  2/20/2019    Executing "use_changer_pos 1"

Setting active sample changer position to 1 (valid sample info found).

10:56:38 AM  2/20/2019    Executing "use_setup "High Q" "Scattering""

Setting active setup to High Q and scan type to Scattering.

10:56:41 AM  2/20/2019    Executing "set_table_scan_title"

Automatically generating
scan title for table scan to:
open(IC: TwoConfigI  S: High Q  P:[])


10:56:41 AM  2/20/2019    Executing "do_parameters_start"


10:56:41 AM  2/20/2019    Executing "go_changer_pos"


10:56:41 AM  2/20/2019    Executing "drive sample_x -178.900000"

SPICE Error in drive command: Wed, Feb 20, 2019 [10:56:41 AM] : SPICE Error in Common.lvlib:Common_Commands.lvlib:Drive_Motor_Val_Pairs.vi.

The argument for motor sample_x, "" contains more than one motor position.

..Move aborted.


10:56:41 AM  2/20/2019    Executing "go_setup"


10:56:41 AM  2/20/2019    Executing "go_setup_beam_trap_in"


10:56:41 AM  2/20/2019    Executing "drive attenuator_pos x10k"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -130.00000

Drive completed.


10:56:42 AM  2/20/2019    Executing "drive trap_y_76mm 554.000000 sdd 1.844000"

Driving to the following position: ""

Destination Motor Positions:
motor           position
trap_y_76mm     554.00000
flange_det_dist 1.80000

Drive completed.


10:56:42 AM  2/20/2019    Executing "if @(hv)<0.5 drive hv 1"


10:56:42 AM  2/20/2019    Executing "do_parameters_finish"


10:56:42 AM  2/20/2019    Executing "go_attenuator"


10:56:42 AM  2/20/2019    Executing "drive attenuator_pos open"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -449.00000

Drive completed.


10:56:43 AM  2/20/2019    Executing "table_scan_counting_initialize"

Initializing counting for current table scan command.

10:56:43 AM  2/20/2019    Executing "scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)"


# scan = 3
# date = 2/20/2019
# time = 10:56:43 AM
# experiment = 
# experiment_number = 0
# ipts_number = undefined
# cycle_number = undefined
# command = scan n=@(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# builtin_command = scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# users = 
# local_contact = 
# scan_title = open(IC: TwoConfigI  S: High Q  P:[])
# samplename = open
# sampletype = Open Beam
# preset_type = normal 
# preset_channel = time
# preset_value = 2.000000
# def_x = Pt.
# def_y = 
# col_headers = 
#   Pt.       time   detector    monitor selector_speed selector_tilt    nguides attenuator_pos beam_trap_x       dcal detector_trans flange_det_dist         hv trap_y_101mm trap_y_25mm trap_y_50mm trap_y_76mm
      1      2.559   1403.000    509.000  5652.7184    -0.0193     4.0000  -448.9999    79.0008     0.0000   400.0001     1.7993     0.9978     0.9998     0.9980     0.9993   553.999
# Footer Info = Add information here
# 10:56:46 AM  2/20/2019   scan completed.

10:56:46 AM  2/20/2019    Executing "table_scan_counting_finalize"

Finalizing counting for current table scan command.

10:56:46 AM  2/20/2019    Executing "go_attenuator_non_open"


10:56:46 AM  2/20/2019    Executing "drive attenuator_pos x10k"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -130.00000

Drive completed.


10:56:46 AM  2/20/2019    Executing "reset_active_changer_pos_data"

Resetting active changer position data.
10:56:46 AM  2/20/2019    Executing "table_scan_finalize 3"

Finalizing info for next table scan command.

10:56:47 AM  2/20/2019    Executing "do_table_scan 2 "High Q" "Scattering" 4"


10:56:47 AM  2/20/2019    Executing "table_scan_initialize 4"

Initializing info for next table scan command.

10:56:47 AM  2/20/2019    Executing "do_table_scan 2 "High Q" "Scattering""


10:56:47 AM  2/20/2019    Executing "use_changer_pos 2"

Setting active sample changer position to 2 (valid sample info found).

10:56:47 AM  2/20/2019    Executing "use_setup "High Q" "Scattering""

Setting active setup to High Q and scan type to Scattering.

10:56:49 AM  2/20/2019    Executing "set_table_scan_title"

Automatically generating
scan title for table scan to:
H2O(IC: TwoConfigI  S: High Q  P:[])


10:56:49 AM  2/20/2019    Executing "do_parameters_start"


10:56:50 AM  2/20/2019    Executing "go_changer_pos"


10:56:50 AM  2/20/2019    Executing "drive sample_x -128.100000"

SPICE Error in drive command: Wed, Feb 20, 2019 [10:56:50 AM] : SPICE Error in Common.lvlib:Common_Commands.lvlib:Drive_Motor_Val_Pairs.vi.

The argument for motor sample_x, "" contains more than one motor position.

..Move aborted.


10:56:50 AM  2/20/2019    Executing "go_setup"


10:56:50 AM  2/20/2019    Executing "go_setup_beam_trap_in"


10:56:50 AM  2/20/2019    Executing "if @(hv)<0.5 drive hv 1"


10:56:50 AM  2/20/2019    Executing "do_parameters_finish"


10:56:50 AM  2/20/2019    Executing "go_attenuator"


10:56:51 AM  2/20/2019    Executing "drive attenuator_pos open"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -449.00000

Drive completed.


10:56:51 AM  2/20/2019    Executing "table_scan_counting_initialize"

Initializing counting for current table scan command.

10:56:51 AM  2/20/2019    Executing "scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)"


# scan = 4
# date = 2/20/2019
# time = 10:56:51 AM
# experiment = 
# experiment_number = 0
# ipts_number = undefined
# cycle_number = undefined
# command = scan n=@(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# builtin_command = scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# users = 
# local_contact = 
# scan_title = H2O(IC: TwoConfigI  S: High Q  P:[])
# samplename = H2O
# sampletype = Sample
# preset_type = normal 
# preset_channel = time
# preset_value = 2.000000
# def_x = Pt.
# def_y = 
# col_headers = 
#   Pt.       time   detector    monitor selector_speed selector_tilt    nguides attenuator_pos beam_trap_x       dcal detector_trans flange_det_dist         hv trap_y_101mm trap_y_25mm trap_y_50mm trap_y_76mm
      1      2.381   1094.000    526.000  5652.7184    -0.0193     4.0000  -449.0284    79.0008     0.0000   400.0001     1.7993     0.9978     0.9998     0.9980     0.9993   553.999
# Footer Info = Add information here
# 10:56:54 AM  2/20/2019   scan completed.

10:56:54 AM  2/20/2019    Executing "table_scan_counting_finalize"

Finalizing counting for current table scan command.

10:56:55 AM  2/20/2019    Executing "go_attenuator_non_open"


10:56:55 AM  2/20/2019    Executing "drive attenuator_pos x10k"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -130.00000

Drive completed.


10:56:55 AM  2/20/2019    Executing "reset_active_changer_pos_data"

Resetting active changer position data.
10:56:55 AM  2/20/2019    Executing "table_scan_finalize 4"

Finalizing info for next table scan command.

10:56:55 AM  2/20/2019    Executing "drive attenuator_pos close"
                          Derived from "attclose"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -7.00000

Drive completed.


10:56:55 AM  2/20/2019    Executing "go_changer_park"

Park position use not enabled for current sample changer.
10:56:56 AM  2/20/2019    Executing "let __active_table_scans.in_progress "0""

Setting variable "__active_table_scans.in_progress" (current value = "1.000000") to "0.000000".

10:57:24 AM  2/20/2019    Executing "let __active_table_scans.in_progress "0""

Setting variable "__active_table_scans.in_progress" (current value = "0.000000") to "0.000000".

Abort issued!!
The following error messages were obtained while restoring the experiment status:

The specified default counting channel, , is not a valid counter channel.

# 2/20/2019 11:09:15 AM	At GP-SANS the PLC has registered a Vacuum Alarm.

11:10:52 AM  2/20/2019    Executing "comment "--------------------Begin Table Scans/Sample Scans Preamble""

COMMENT:
--------------------Begin Table Scans/Sample Scans Preamble


11:10:52 AM  2/20/2019    Executing "reset_active_scan_data"

Resetting active scan data.
11:10:54 AM  2/20/2019    Executing "scantitle """

Setting the scantitle to:



11:10:54 AM  2/20/2019    Executing "set_sample_info_sample_changer "Flat changer" 8"

Setting sample info sample changer name to Flat changer 
with 8 changer positions.

11:10:54 AM  2/20/2019    Executing "set_sample_info_instrument_config "TwoConfigI" "Mid Q,High Q""

Setting sample info instrument configuration name to TwoConfigI.
 
11:10:54 AM  2/20/2019    Executing "set_sample_info_parameter_config "No Parameters" "" """

Setting sample info parameter configuration name to No Parameters.
 
11:10:55 AM  2/20/2019    Executing "set_sample_info_setup_order "Mid Q,High Q""

Setting sample info setup order to "Mid Q,High Q".

11:10:55 AM  2/20/2019    Executing "set_sample_info_scan_order "Setup Order""

Setting sample info scan order to "Setup Order".
 
11:10:55 AM  2/20/2019    Executing "set_sample_info_do_transmission_scans "false""

Setting sample info do_transmission_scans to "false".

11:10:55 AM  2/20/2019    Executing "set_sample_info_specify_frames "false""

Setting sample info specify_frames to "false".
 
11:10:55 AM  2/20/2019    Executing "set_sample_info_background_columns_names "Cell Thickness (mm)""

Setting sample info background columns names to "Cell Thickness (mm)".
 
11:10:55 AM  2/20/2019    Executing "set_sample_info_background_columns_default_values "True""

Setting sample info background columns default values to "True".
 
11:10:55 AM  2/20/2019    Executing "set_sample_info_sample_columns_names """

Setting sample info sample columns names to "".
 
11:10:55 AM  2/20/2019    Executing "set_sample_info_sample_columns_default_values """

Setting sample info sample columns default values to "".
 
11:10:55 AM  2/20/2019    Executing "set_sample_info_sample_id 1 """

Setting sample info sample id to  
for changer position 1.

11:10:55 AM  2/20/2019    Executing "set_sample_info_sample_name 1 "open""

Setting sample info sample name to open 
for changer position 1.

11:10:56 AM  2/20/2019    Executing "set_sample_info_sample_thickness 1 "1.000000""

Setting sample info sample thickness to 1.000000 mm 
for changer position 1.

11:10:56 AM  2/20/2019    Executing "set_sample_info_sample_columns_values 1 ",""

Setting sample info sample columns values to "," 
for changer position 1.

11:10:56 AM  2/20/2019    Executing "set_sample_info_background_columns_values 1 "True""

Setting sample info background columns values to "True" 
for changer position 1.

11:10:56 AM  2/20/2019    Executing "set_sample_info_sample_type 1 "Open Beam""

Setting sample info sample type to Open Beam 
for changer position 1.

11:10:56 AM  2/20/2019    Executing "set_sample_info_do_scan 1 "true""

Setting sample info do_scan value to true 
for changer position 1.

11:10:56 AM  2/20/2019    Executing "set_sample_info_scan_times 1 "2.000000,2.000000""

Setting sample info scan times values to "2.000000,2.000000" 
for changer position 1.

11:10:56 AM  2/20/2019    Executing "set_sample_info_frame_counts 1 "1,1""

Setting sample info frame counts values to "1,1" 
for changer position 1.

11:10:56 AM  2/20/2019    Executing "set_sample_info_parameter_columns_values 1 """

Setting sample info parameter columns values to "" 
for changer position 1.

11:10:56 AM  2/20/2019    Executing "set_sample_info_sample_id 2 """

Setting sample info sample id to  
for changer position 2.

11:10:57 AM  2/20/2019    Executing "set_sample_info_sample_name 2 "H2O""

Setting sample info sample name to H2O 
for changer position 2.

11:10:57 AM  2/20/2019    Executing "set_sample_info_sample_thickness 2 "1.000000""

Setting sample info sample thickness to 1.000000 mm 
for changer position 2.

11:10:57 AM  2/20/2019    Executing "set_sample_info_sample_columns_values 2 """

Setting sample info sample columns values to "" 
for changer position 2.

11:10:57 AM  2/20/2019    Executing "set_sample_info_background_columns_values 2 "True""

Setting sample info background columns values to "True" 
for changer position 2.

11:10:57 AM  2/20/2019    Executing "set_sample_info_sample_type 2 "Sample""

Setting sample info sample type to Sample 
for changer position 2.

11:10:57 AM  2/20/2019    Executing "set_sample_info_do_scan 2 "true""

Setting sample info do_scan value to true 
for changer position 2.

11:10:57 AM  2/20/2019    Executing "set_sample_info_scan_times 2 "2.000000,2.000000""

Setting sample info scan times values to "2.000000,2.000000" 
for changer position 2.

11:10:57 AM  2/20/2019    Executing "set_sample_info_frame_counts 2 "1,1""

Setting sample info frame counts values to "1,1" 
for changer position 2.

11:10:57 AM  2/20/2019    Executing "set_sample_info_parameter_columns_values 2 """

Setting sample info parameter columns values to "" 
for changer position 2.

11:10:57 AM  2/20/2019    Executing "set_sample_info_sample_id 3 """

Setting sample info sample id to  
for changer position 3.

11:10:58 AM  2/20/2019    Executing "set_sample_info_sample_name 3 "AgBeh""

Setting sample info sample name to AgBeh 
for changer position 3.

11:10:58 AM  2/20/2019    Executing "set_sample_info_sample_thickness 3 "1.000000""

Setting sample info sample thickness to 1.000000 mm 
for changer position 3.

11:10:58 AM  2/20/2019    Executing "set_sample_info_sample_columns_values 3 """

Setting sample info sample columns values to "" 
for changer position 3.

11:10:58 AM  2/20/2019    Executing "set_sample_info_background_columns_values 3 "True""

Setting sample info background columns values to "True" 
for changer position 3.

11:10:58 AM  2/20/2019    Executing "set_sample_info_sample_type 3 "Sample""

Setting sample info sample type to Sample 
for changer position 3.

11:10:58 AM  2/20/2019    Executing "set_sample_info_do_scan 3 "false""

Setting sample info do_scan value to false 
for changer position 3.

11:10:58 AM  2/20/2019    Executing "set_sample_info_scan_times 3 "0.000000,300.000000""

Setting sample info scan times values to "0.000000,300.000000" 
for changer position 3.

11:10:58 AM  2/20/2019    Executing "set_sample_info_frame_counts 3 "1,1""

Setting sample info frame counts values to "1,1" 
for changer position 3.

11:10:58 AM  2/20/2019    Executing "set_sample_info_parameter_columns_values 3 """

Setting sample info parameter columns values to "" 
for changer position 3.

11:10:58 AM  2/20/2019    Executing "set_sample_info_sample_id 4 """

Setting sample info sample id to  
for changer position 4.

11:10:58 AM  2/20/2019    Executing "set_sample_info_sample_name 4 "5""

Setting sample info sample name to 5 
for changer position 4.

11:10:59 AM  2/20/2019    Executing "set_sample_info_sample_thickness 4 "1.000000""

Setting sample info sample thickness to 1.000000 mm 
for changer position 4.

11:10:59 AM  2/20/2019    Executing "set_sample_info_sample_columns_values 4 """

Setting sample info sample columns values to "" 
for changer position 4.

11:10:59 AM  2/20/2019    Executing "set_sample_info_background_columns_values 4 "True""

Setting sample info background columns values to "True" 
for changer position 4.

11:10:59 AM  2/20/2019    Executing "set_sample_info_sample_type 4 "Sample""

Setting sample info sample type to Sample 
for changer position 4.

11:10:59 AM  2/20/2019    Executing "set_sample_info_do_scan 4 "false""

Setting sample info do_scan value to false 
for changer position 4.

11:10:59 AM  2/20/2019    Executing "set_sample_info_scan_times 4 "0.000000,300.000000""

Setting sample info scan times values to "0.000000,300.000000" 
for changer position 4.

11:10:59 AM  2/20/2019    Executing "set_sample_info_frame_counts 4 "1,1""

Setting sample info frame counts values to "1,1" 
for changer position 4.

11:10:59 AM  2/20/2019    Executing "set_sample_info_parameter_columns_values 4 """

Setting sample info parameter columns values to "" 
for changer position 4.

11:11:00 AM  2/20/2019    Executing "set_sample_info_sample_id 5 """

Setting sample info sample id to  
for changer position 5.

11:11:00 AM  2/20/2019    Executing "set_sample_info_sample_name 5 """

Setting sample info sample name to  
for changer position 5.

11:11:00 AM  2/20/2019    Executing "set_sample_info_sample_thickness 5 "1.000000""

Setting sample info sample thickness to 1.000000 mm 
for changer position 5.

11:11:00 AM  2/20/2019    Executing "set_sample_info_sample_columns_values 5 """

Setting sample info sample columns values to "" 
for changer position 5.

11:11:00 AM  2/20/2019    Executing "set_sample_info_background_columns_values 5 "True""

Setting sample info background columns values to "True" 
for changer position 5.

11:11:00 AM  2/20/2019    Executing "set_sample_info_sample_type 5 "Sample""

Setting sample info sample type to Sample 
for changer position 5.

11:11:00 AM  2/20/2019    Executing "set_sample_info_do_scan 5 "false""

Setting sample info do_scan value to false 
for changer position 5.

11:11:00 AM  2/20/2019    Executing "set_sample_info_scan_times 5 "0.000000,300.000000""

Setting sample info scan times values to "0.000000,300.000000" 
for changer position 5.

11:11:00 AM  2/20/2019    Executing "set_sample_info_frame_counts 5 "1,1""

Setting sample info frame counts values to "1,1" 
for changer position 5.

11:11:00 AM  2/20/2019    Executing "set_sample_info_parameter_columns_values 5 """

Setting sample info parameter columns values to "" 
for changer position 5.

11:11:01 AM  2/20/2019    Executing "set_sample_info_sample_id 6 """

Setting sample info sample id to  
for changer position 6.

11:11:01 AM  2/20/2019    Executing "set_sample_info_sample_name 6 """

Setting sample info sample name to  
for changer position 6.

11:11:01 AM  2/20/2019    Executing "set_sample_info_sample_thickness 6 "1.000000""

Setting sample info sample thickness to 1.000000 mm 
for changer position 6.

11:11:01 AM  2/20/2019    Executing "set_sample_info_sample_columns_values 6 """

Setting sample info sample columns values to "" 
for changer position 6.

11:11:01 AM  2/20/2019    Executing "set_sample_info_background_columns_values 6 "True""

Setting sample info background columns values to "True" 
for changer position 6.

11:11:01 AM  2/20/2019    Executing "set_sample_info_sample_type 6 "Sample""

Setting sample info sample type to Sample 
for changer position 6.

11:11:01 AM  2/20/2019    Executing "set_sample_info_do_scan 6 "false""

Setting sample info do_scan value to false 
for changer position 6.

11:11:01 AM  2/20/2019    Executing "set_sample_info_scan_times 6 "0.000000,300.000000""

Setting sample info scan times values to "0.000000,300.000000" 
for changer position 6.

11:11:01 AM  2/20/2019    Executing "set_sample_info_frame_counts 6 "1,1""

Setting sample info frame counts values to "1,1" 
for changer position 6.

11:11:01 AM  2/20/2019    Executing "set_sample_info_parameter_columns_values 6 """

Setting sample info parameter columns values to "" 
for changer position 6.

11:11:02 AM  2/20/2019    Executing "set_sample_info_sample_id 7 """

Setting sample info sample id to  
for changer position 7.

11:11:02 AM  2/20/2019    Executing "set_sample_info_sample_name 7 """

Setting sample info sample name to  
for changer position 7.

11:11:02 AM  2/20/2019    Executing "set_sample_info_sample_thickness 7 "1.000000""

Setting sample info sample thickness to 1.000000 mm 
for changer position 7.

11:11:02 AM  2/20/2019    Executing "set_sample_info_sample_columns_values 7 """

Setting sample info sample columns values to "" 
for changer position 7.

11:11:02 AM  2/20/2019    Executing "set_sample_info_background_columns_values 7 "True""

Setting sample info background columns values to "True" 
for changer position 7.

11:11:02 AM  2/20/2019    Executing "set_sample_info_sample_type 7 "Sample""

Setting sample info sample type to Sample 
for changer position 7.

11:11:02 AM  2/20/2019    Executing "set_sample_info_do_scan 7 "false""

Setting sample info do_scan value to false 
for changer position 7.

11:11:02 AM  2/20/2019    Executing "set_sample_info_scan_times 7 "0.000000,300.000000""

Setting sample info scan times values to "0.000000,300.000000" 
for changer position 7.

11:11:02 AM  2/20/2019    Executing "set_sample_info_frame_counts 7 "1,1""

Setting sample info frame counts values to "1,1" 
for changer position 7.

11:11:02 AM  2/20/2019    Executing "set_sample_info_parameter_columns_values 7 """

Setting sample info parameter columns values to "" 
for changer position 7.

11:11:03 AM  2/20/2019    Executing "set_sample_info_sample_id 8 """

Setting sample info sample id to  
for changer position 8.

11:11:03 AM  2/20/2019    Executing "set_sample_info_sample_name 8 "R10_20""

Setting sample info sample name to R10_20 
for changer position 8.

11:11:03 AM  2/20/2019    Executing "set_sample_info_sample_thickness 8 "1.000000""

Setting sample info sample thickness to 1.000000 mm 
for changer position 8.

11:11:03 AM  2/20/2019    Executing "set_sample_info_sample_columns_values 8 """

Setting sample info sample columns values to "" 
for changer position 8.

11:11:03 AM  2/20/2019    Executing "set_sample_info_background_columns_values 8 "True""

Setting sample info background columns values to "True" 
for changer position 8.

11:11:03 AM  2/20/2019    Executing "set_sample_info_sample_type 8 "Sample""

Setting sample info sample type to Sample 
for changer position 8.

11:11:03 AM  2/20/2019    Executing "set_sample_info_do_scan 8 "false""

Setting sample info do_scan value to false 
for changer position 8.

11:11:03 AM  2/20/2019    Executing "set_sample_info_scan_times 8 "0.000000,300.000000""

Setting sample info scan times values to "0.000000,300.000000" 
for changer position 8.

11:11:04 AM  2/20/2019    Executing "set_sample_info_frame_counts 8 "1,1""

Setting sample info frame counts values to "1,1" 
for changer position 8.

11:11:04 AM  2/20/2019    Executing "set_sample_info_parameter_columns_values 8 """

Setting sample info parameter columns values to "" 
for changer position 8.

11:11:04 AM  2/20/2019    Executing "use_sample_changer "Flat changer""

Setting active sample changer to Flat changer.

11:11:04 AM  2/20/2019    Executing "use_instrument_config "TwoConfigI""

Setting active instrument config to TwoConfigI.

11:11:05 AM  2/20/2019    Executing "use_parameter_config "No Parameters""

Setting active parameter config to No Parameters.

11:11:05 AM  2/20/2019    Executing "comment "--------------------End Table Scans/Sample Scans Preamble""

COMMENT:
--------------------End Table Scans/Sample Scans Preamble


11:11:05 AM  2/20/2019    Executing "reset_active_table_scans"

Resetting active table scan command info.
11:11:05 AM  2/20/2019    Executing "set_table_scan_command_info "do_table_scan 1 \22Mid Q\22 \22Scattering\22 1" 1 "open" "Mid Q" "Scattering" 2.000000 1 2.000000"

Setting  info for next table scan command.

11:11:05 AM  2/20/2019    Executing "set_table_scan_command_info "do_table_scan 2 \22Mid Q\22 \22Scattering\22 2" 2 "H2O" "Mid Q" "Scattering" 2.000000 1 2.000000"

Setting  info for next table scan command.

11:11:05 AM  2/20/2019    Executing "set_table_scan_command_info "do_table_scan 1 \22High Q\22 \22Scattering\22 3" 1 "open" "High Q" "Scattering" 2.000000 1 2.000000"

Setting  info for next table scan command.

11:11:05 AM  2/20/2019    Executing "set_table_scan_command_info "do_table_scan 2 \22High Q\22 \22Scattering\22 4" 2 "H2O" "High Q" "Scattering" 2.000000 1 2.000000"

Setting  info for next table scan command.

11:11:05 AM  2/20/2019    Executing "let __active_table_scans.in_progress "1""

Setting variable "__active_table_scans.in_progress" (current value = "0") to "1.000000".

11:11:06 AM  2/20/2019    Executing "do_table_scan 1 "Mid Q" "Scattering" 1"


11:11:06 AM  2/20/2019    Executing "table_scan_initialize 1"

Initializing info for next table scan command.

11:11:06 AM  2/20/2019    Executing "do_table_scan 1 "Mid Q" "Scattering""


11:11:06 AM  2/20/2019    Executing "use_changer_pos 1"

Setting active sample changer position to 1 (valid sample info found).

11:11:06 AM  2/20/2019    Executing "use_setup "Mid Q" "Scattering""

Setting active setup to Mid Q and scan type to Scattering.

11:11:08 AM  2/20/2019    Executing "set_table_scan_title"

Automatically generating
scan title for table scan to:
open(IC: TwoConfigI  S: Mid Q  P:[])


11:11:08 AM  2/20/2019    Executing "do_parameters_start"


11:11:08 AM  2/20/2019    Executing "go_changer_pos"


11:11:08 AM  2/20/2019    Executing "drive sample_x -178.900000"

SPICE Error in drive command: Wed, Feb 20, 2019 [11:11:08 AM] : SPICE Error in Common.lvlib:Common_Commands.lvlib:Drive_Motor_Val_Pairs.vi.

The argument for motor sample_x, "" contains more than one motor position.

..Move aborted.


11:11:08 AM  2/20/2019    Executing "go_setup"


11:11:08 AM  2/20/2019    Executing "go_setup_beam_trap_in"


11:11:08 AM  2/20/2019    Executing "drive trap_y_76mm 552.000000 sdd 8.844000"

Driving to the following position: ""

Destination Motor Positions:
motor           position
trap_y_76mm     552.00000
flange_det_dist 8.80000

Drive completed.


11:11:10 AM  2/20/2019    Executing "if @(hv)<0.5 drive hv 1"


11:11:10 AM  2/20/2019    Executing "do_parameters_finish"


11:11:10 AM  2/20/2019    Executing "go_attenuator"


11:11:10 AM  2/20/2019    Executing "drive attenuator_pos open"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -449.00000

Drive completed.


11:11:10 AM  2/20/2019    Executing "table_scan_counting_initialize"

Initializing counting for current table scan command.

11:11:11 AM  2/20/2019    Executing "scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)"


# scan = 1
# date = 2/20/2019
# time = 11:11:11 AM
# experiment = 
# experiment_number = 0
# ipts_number = undefined
# cycle_number = undefined
# command = scan n=@(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# builtin_command = scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# users = 
# local_contact = 
# scan_title = open(IC: TwoConfigI  S: Mid Q  P:[])
# samplename = open
# sampletype = Open Beam
# preset_type = normal 
# preset_channel = time
# preset_value = 2.000000
# def_x = Pt.
# def_y = 
# col_headers = 
#   Pt.       time   detector    monitor selector_speed selector_tilt    nguides attenuator_pos beam_trap_x       dcal detector_trans flange_det_dist         hv trap_y_101mm trap_y_25mm trap_y_50mm trap_y_76mm
      1      2.706   1402.000    549.000  5652.7184    -0.0193     4.0000  -449.0011    79.0008     0.0000   400.0001     8.7973     0.9978     0.9998     0.9980     0.9993   551.997
# Footer Info = Add information here
# 11:11:15 AM  2/20/2019   scan completed.

11:11:15 AM  2/20/2019    Executing "table_scan_counting_finalize"

Finalizing counting for current table scan command.

11:11:15 AM  2/20/2019    Executing "go_attenuator_non_open"


11:11:15 AM  2/20/2019    Executing "drive attenuator_pos x10k"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -130.00000

Drive completed.


11:11:15 AM  2/20/2019    Executing "reset_active_changer_pos_data"

Resetting active changer position data.
11:11:16 AM  2/20/2019    Executing "table_scan_finalize 1"

Finalizing info for next table scan command.

11:11:16 AM  2/20/2019    Executing "do_table_scan 2 "Mid Q" "Scattering" 2"


11:11:16 AM  2/20/2019    Executing "table_scan_initialize 2"

Initializing info for next table scan command.

11:11:16 AM  2/20/2019    Executing "do_table_scan 2 "Mid Q" "Scattering""


11:11:16 AM  2/20/2019    Executing "use_changer_pos 2"

Setting active sample changer position to 2 (valid sample info found).

11:11:17 AM  2/20/2019    Executing "use_setup "Mid Q" "Scattering""

Setting active setup to Mid Q and scan type to Scattering.

11:11:22 AM  2/20/2019    Executing "set_table_scan_title"

Automatically generating
scan title for table scan to:
H2O(IC: TwoConfigI  S: Mid Q  P:[])


11:11:22 AM  2/20/2019    Executing "do_parameters_start"


11:11:22 AM  2/20/2019    Executing "go_changer_pos"


11:11:23 AM  2/20/2019    Executing "drive sample_x -128.100000"

SPICE Error in drive command: Wed, Feb 20, 2019 [11:11:23 AM] : SPICE Error in Common.lvlib:Common_Commands.lvlib:Drive_Motor_Val_Pairs.vi.

The argument for motor sample_x, "" contains more than one motor position.

..Move aborted.


11:11:23 AM  2/20/2019    Executing "go_setup"


11:11:23 AM  2/20/2019    Executing "go_setup_beam_trap_in"


11:11:23 AM  2/20/2019    Executing "drive attenuator_pos x10k"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -130.00000

Drive completed.


11:11:24 AM  2/20/2019    Executing "if @(hv)<0.5 drive hv 1"


11:11:24 AM  2/20/2019    Executing "do_parameters_finish"


11:11:25 AM  2/20/2019    Executing "go_attenuator"


11:11:25 AM  2/20/2019    Executing "drive attenuator_pos open"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -449.00000

Drive completed.


11:11:25 AM  2/20/2019    Executing "table_scan_counting_initialize"

Initializing counting for current table scan command.

11:11:26 AM  2/20/2019    Executing "scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)"


# scan = 2
# date = 2/20/2019
# time = 11:11:26 AM
# experiment = 
# experiment_number = 0
# ipts_number = undefined
# cycle_number = undefined
# command = scan n=@(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# builtin_command = scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# users = 
# local_contact = 
# scan_title = H2O(IC: TwoConfigI  S: Mid Q  P:[])
# samplename = H2O
# sampletype = Sample
# preset_type = normal 
# preset_channel = time
# preset_value = 2.000000
# def_x = Pt.
# def_y = 
# col_headers = 
#   Pt.       time   detector    monitor selector_speed selector_tilt    nguides attenuator_pos beam_trap_x       dcal detector_trans flange_det_dist         hv trap_y_101mm trap_y_25mm trap_y_50mm trap_y_76mm
      1      2.378   1102.000    504.000  5652.7184    -0.0193     4.0000  -448.9866    79.0008     0.0000   400.0001     8.7973     0.9978     0.9998     0.9980     0.9993   551.997
# Footer Info = Add information here
# 11:11:29 AM  2/20/2019   scan completed.

11:11:29 AM  2/20/2019    Executing "table_scan_counting_finalize"

Finalizing counting for current table scan command.

11:11:29 AM  2/20/2019    Executing "go_attenuator_non_open"


11:11:29 AM  2/20/2019    Executing "drive attenuator_pos x10k"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -130.00000

Drive completed.


11:11:30 AM  2/20/2019    Executing "reset_active_changer_pos_data"

Resetting active changer position data.
11:11:30 AM  2/20/2019    Executing "table_scan_finalize 2"

Finalizing info for next table scan command.

11:11:30 AM  2/20/2019    Executing "do_table_scan 1 "High Q" "Scattering" 3"


11:11:30 AM  2/20/2019    Executing "table_scan_initialize 3"

Initializing info for next table scan command.

11:11:31 AM  2/20/2019    Executing "do_table_scan 1 "High Q" "Scattering""


11:11:31 AM  2/20/2019    Executing "use_changer_pos 1"

Setting active sample changer position to 1 (valid sample info found).

11:11:31 AM  2/20/2019    Executing "use_setup "High Q" "Scattering""

Setting active setup to High Q and scan type to Scattering.

11:11:37 AM  2/20/2019    Executing "set_table_scan_title"

Automatically generating
scan title for table scan to:
open(IC: TwoConfigI  S: High Q  P:[])


11:11:37 AM  2/20/2019    Executing "do_parameters_start"


11:11:37 AM  2/20/2019    Executing "go_changer_pos"


11:11:37 AM  2/20/2019    Executing "drive sample_x -178.900000"

SPICE Error in drive command: Wed, Feb 20, 2019 [11:11:37 AM] : SPICE Error in Common.lvlib:Common_Commands.lvlib:Drive_Motor_Val_Pairs.vi.

The argument for motor sample_x, "" contains more than one motor position.

..Move aborted.


11:11:38 AM  2/20/2019    Executing "go_setup"


11:11:38 AM  2/20/2019    Executing "go_setup_beam_trap_in"


11:11:38 AM  2/20/2019    Executing "drive attenuator_pos x10k"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -130.00000

Drive completed.


11:11:38 AM  2/20/2019    Executing "drive trap_y_76mm 554.000000 sdd 1.844000"

Driving to the following position: ""

Destination Motor Positions:
motor           position
trap_y_76mm     554.00000
flange_det_dist 1.80000

Drive completed.


11:11:40 AM  2/20/2019    Executing "if @(hv)<0.5 drive hv 1"


11:11:40 AM  2/20/2019    Executing "do_parameters_finish"


11:11:40 AM  2/20/2019    Executing "go_attenuator"


11:11:40 AM  2/20/2019    Executing "drive attenuator_pos open"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -449.00000

Drive completed.


11:11:40 AM  2/20/2019    Executing "table_scan_counting_initialize"

Initializing counting for current table scan command.

11:11:41 AM  2/20/2019    Executing "scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)"


# scan = 3
# date = 2/20/2019
# time = 11:11:41 AM
# experiment = 
# experiment_number = 0
# ipts_number = undefined
# cycle_number = undefined
# command = scan n=@(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# builtin_command = scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# users = 
# local_contact = 
# scan_title = open(IC: TwoConfigI  S: High Q  P:[])
# samplename = open
# sampletype = Open Beam
# preset_type = normal 
# preset_channel = time
# preset_value = 2.000000
# def_x = Pt.
# def_y = 
# col_headers = 
#   Pt.       time   detector    monitor selector_speed selector_tilt    nguides attenuator_pos beam_trap_x       dcal detector_trans flange_det_dist         hv trap_y_101mm trap_y_25mm trap_y_50mm trap_y_76mm
      1      2.420   1394.000    501.000  5652.7184    -0.0193     4.0000  -449.0080    79.0008     0.0000   400.0001     1.7976     0.9978     0.9998     0.9980     0.9993   554.001
# Footer Info = Add information here
# 11:11:44 AM  2/20/2019   scan completed.

11:11:44 AM  2/20/2019    Executing "table_scan_counting_finalize"

Finalizing counting for current table scan command.

11:11:44 AM  2/20/2019    Executing "go_attenuator_non_open"


11:11:44 AM  2/20/2019    Executing "drive attenuator_pos x10k"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -130.00000

Drive completed.


11:11:45 AM  2/20/2019    Executing "reset_active_changer_pos_data"

Resetting active changer position data.
11:11:45 AM  2/20/2019    Executing "table_scan_finalize 3"

Finalizing info for next table scan command.

11:11:45 AM  2/20/2019    Executing "do_table_scan 2 "High Q" "Scattering" 4"


11:11:45 AM  2/20/2019    Executing "table_scan_initialize 4"

Initializing info for next table scan command.

11:11:46 AM  2/20/2019    Executing "do_table_scan 2 "High Q" "Scattering""


11:11:46 AM  2/20/2019    Executing "use_changer_pos 2"

Setting active sample changer position to 2 (valid sample info found).

11:11:46 AM  2/20/2019    Executing "use_setup "High Q" "Scattering""

Setting active setup to High Q and scan type to Scattering.

11:11:51 AM  2/20/2019    Executing "set_table_scan_title"

Automatically generating
scan title for table scan to:
H2O(IC: TwoConfigI  S: High Q  P:[])


11:11:51 AM  2/20/2019    Executing "do_parameters_start"


11:11:51 AM  2/20/2019    Executing "go_changer_pos"


11:11:51 AM  2/20/2019    Executing "drive sample_x -128.100000"

SPICE Error in drive command: Wed, Feb 20, 2019 [11:11:51 AM] : SPICE Error in Common.lvlib:Common_Commands.lvlib:Drive_Motor_Val_Pairs.vi.

The argument for motor sample_x, "" contains more than one motor position.

..Move aborted.


11:11:51 AM  2/20/2019    Executing "go_setup"


11:11:52 AM  2/20/2019    Executing "go_setup_beam_trap_in"


11:11:52 AM  2/20/2019    Executing "drive attenuator_pos x10k"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -130.00000

Drive completed.


11:11:52 AM  2/20/2019    Executing "if @(hv)<0.5 drive hv 1"


11:11:52 AM  2/20/2019    Executing "do_parameters_finish"


11:11:52 AM  2/20/2019    Executing "go_attenuator"


11:11:53 AM  2/20/2019    Executing "drive attenuator_pos open"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -449.00000

Drive completed.


11:11:53 AM  2/20/2019    Executing "table_scan_counting_initialize"

Initializing counting for current table scan command.

11:11:53 AM  2/20/2019    Executing "scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)"


# scan = 4
# date = 2/20/2019
# time = 11:11:53 AM
# experiment = 
# experiment_number = 0
# ipts_number = undefined
# cycle_number = undefined
# command = scan n=@(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# builtin_command = scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# users = 
# local_contact = 
# scan_title = H2O(IC: TwoConfigI  S: High Q  P:[])
# samplename = H2O
# sampletype = Sample
# preset_type = normal 
# preset_channel = time
# preset_value = 2.000000
# def_x = Pt.
# def_y = 
# col_headers = 
#   Pt.       time   detector    monitor selector_speed selector_tilt    nguides attenuator_pos beam_trap_x       dcal detector_trans flange_det_dist         hv trap_y_101mm trap_y_25mm trap_y_50mm trap_y_76mm
      1      2.681   1655.000    555.000  5652.7184    -0.0193     4.0000  -448.9973    79.0008     0.0000   400.0001     1.7976     0.9978     0.9998     0.9980     0.9993   554.001
# Footer Info = Add information here
# 11:11:56 AM  2/20/2019   scan completed.

11:11:56 AM  2/20/2019    Executing "table_scan_counting_finalize"

Finalizing counting for current table scan command.

11:11:57 AM  2/20/2019    Executing "go_attenuator_non_open"


11:11:57 AM  2/20/2019    Executing "drive attenuator_pos x10k"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -130.00000

Drive completed.


11:11:57 AM  2/20/2019    Executing "reset_active_changer_pos_data"

Resetting active changer position data.
11:11:58 AM  2/20/2019    Executing "table_scan_finalize 4"

Finalizing info for next table scan command.

11:11:58 AM  2/20/2019    Executing "drive attenuator_pos close"
                          Derived from "attclose"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -7.00000

Drive completed.


11:11:58 AM  2/20/2019    Executing "go_changer_park"

Park position use not enabled for current sample changer.
11:11:58 AM  2/20/2019    Executing "let __active_table_scans.in_progress "0""

Setting variable "__active_table_scans.in_progress" (current value = "1.000000") to "0.000000".

11:14:13 AM  2/20/2019    Executing "let __active_table_scans.in_progress "0""

The following error messages were obtained while restoring the experiment status:

The specified default counting channel, , is not a valid counter channel.

# 2/20/2019 12:45:44 PM	At GP-SANS the PLC has registered a Vacuum Alarm.

12:46:02 PM  2/20/2019    Executing "let __active_table_scans.in_progress "0""

Setting variable "__active_table_scans.in_progress" (current value = "") to "0.000000".

Abort issued!!
The following error messages were obtained while restoring the experiment status:

The specified default counting channel, , is not a valid counter channel.

# 2/20/2019 12:46:48 PM	At GP-SANS the PLC has registered a Vacuum Alarm.

12:46:59 PM  2/20/2019    Executing "let __active_table_scans.in_progress "0""

Setting variable "__active_table_scans.in_progress" (current value = "") to "0.000000".

Abort issued!!
The following error messages were obtained while restoring the experiment status:

The specified default counting channel, , is not a valid counter channel.

# 2/20/2019 1:08:51 PM	At GP-SANS the PLC has registered a Vacuum Alarm.

1:16:42 PM  2/20/2019    Executing "let __active_table_scans.in_progress "0""

Setting variable "__active_table_scans.in_progress" (current value = "") to "0.000000".

Abort issued!!
The following error messages were obtained while restoring the experiment status:

The specified default counting channel, , is not a valid counter channel.

# 2/20/2019 1:37:18 PM	At GP-SANS the PLC has registered a Vacuum Alarm.

1:37:35 PM  2/20/2019    Executing "let __active_table_scans.in_progress "0""

Setting variable "__active_table_scans.in_progress" (current value = "") to "0.000000".

Abort issued!!
The following error messages were obtained while restoring the experiment status:

The specified default counting channel, , is not a valid counter channel.

# 2/20/2019 1:59:53 PM	At GP-SANS the PLC has registered a Vacuum Alarm.

2:00:02 PM  2/20/2019    Executing "let __active_table_scans.in_progress "0""

Setting variable "__active_table_scans.in_progress" (current value = "") to "0.000000".

Abort issued!!
