Beginning experiment # 456

Proposal ID: "17241"

Cycle Number: "475"

Experiment title: "Long Outage MP"

Users: "Shuo Qian"

Local Contact: "Shuo Qian"

Setting next scan number to 1

Initializing preset/counting configuration:

Preset counting mode is set to normal.

Setting the default preset channel to "time".

Setting the default preset value to 300.000.

The following error messages were obtained while restoring the experiment status:

The specified default counting channel, , is not a valid counter channel.


The username/password request for web access was cancelled or the dialog box timed out.
Web-based control will not function until these are set.  This can be accomplished using the 'webcontrol' command.


11:10:13 PM  9/29/2017    Executing "scantitle "detector dark current reactor off""

Setting the scantitle to:
detector dark current reactor off


11:10:22 PM  9/29/2017    Executing "drive attenuator_pos open"
                          Derived from "attopen"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -449.00000

# Motor is moving but no drive is in progress.Drive completed.


11:10:54 PM  9/29/2017    Executing "drive aperture_x out sample_x out"

Driving to the following position: ""

Destination Motor Positions:
motor           position
aperture_x      -200.00000
sample_x        215.00000

[11:11:12 PM  9/29/2017]     ### Supplemental drive will be attempted for motor sample_x which has a current position of 210.769200.
[11:11:12 PM  9/29/2017]     ### Supplemental drive will be attempted for motor aperture_x which has a current position of -195.623180.
[11:11:12 PM  9/29/2017]     ### Supplemental drive will be attempted for motor sample_x which has a current position of 214.901780.
[11:11:13 PM  9/29/2017]     ### Supplemental drive will be attempted for motor aperture_x which has a current position of -199.896730.
Drive completed.


11:11:40 PM  9/29/2017    Executing "scan preset time 1800000"


# scan = 1
# date = 9/29/2017
# time = 11:11:40 PM
# experiment = Long Outage MP
# experiment_number = 456
# ipts_number = 17241
# cycle_number = 475
# command = scan preset time 1800000
# builtin_command = scan preset time 1800000
# users = Shuo Qian
# local_contact = Shuo Qian
# scan_title = detector dark current reactor off
# samplename = 
# sampletype = Open Beam
# preset_type = normal 
# preset_channel = time
# preset_value = 1800000.000000
# def_x = Pt.
# def_y = 
# col_headers = 
#   Pt.       time    monitor   detector detector_body detector_wing    tumbler selector_speed selector_tilt   chillerp    chiller        sdd    nguides aperture_x attenuator_pos beam_trap_x       dcal det_west_wing_rot flange_det_dist   hum_vert   sample_x trap_y_25mm
      1     36.421      3.000     70.000     43.000     27.000 14618.0609  4444.9000     0.0000    43.9900    44.0000    15.5000     0.0000  -199.9983  -449.0022    81.0000  1140.0007     1.0020    15.4190    17.0000   214.9970   545.000
# Footer Info = Add information here
# 11:12:18 PM  9/29/2017   scan stopped!!

Abort issued!!

11:12:18 PM  9/29/2017    Executing "let __active_table_scans.in_progress "0""

Setting variable "__active_table_scans.in_progress" (current value = "") to "0.000000".

11:12:40 PM  9/29/2017    Executing "scan n 10 preset time 18000"


# scan = 2
# date = 9/29/2017
# time = 11:12:40 PM
# experiment = Long Outage MP
# experiment_number = 456
# ipts_number = 17241
# cycle_number = 475
# command = scan n=10 preset time 18000
# builtin_command = scan n 10 preset time 18000
# users = Shuo Qian
# local_contact = Shuo Qian
# scan_title = detector dark current reactor off
# samplename = 
# sampletype = Open Beam
# preset_type = normal 
# preset_channel = time
# preset_value = 18000.000000
# def_x = Pt.
# def_y = 
# col_headers = 
#   Pt.       time    monitor   detector detector_body detector_wing    tumbler selector_speed selector_tilt   chillerp    chiller        sdd    nguides aperture_x attenuator_pos beam_trap_x       dcal det_west_wing_rot flange_det_dist   hum_vert   sample_x trap_y_25mm
      1  18000.594    661.000  38170.000  25308.000  12862.000 14618.0609  4444.9000     0.0000    44.0000    44.0000    15.5000     0.0000  -199.9983  -449.0022    81.0000  1140.0007     1.0020    15.4190    17.0000   214.9970   545.000
      2  18000.813    249.000  38094.000  25268.000  12826.000 14618.0609  4444.9000     0.0000    44.0000    44.0000    15.5000     0.0000  -199.9983  -449.0022    81.0000  1140.0007     1.0020    15.4190    17.0000   214.9970   545.000
      3  18000.953    105.000  37661.000  24864.000  12797.000 14618.0609  4444.9000     0.0000    44.0000    44.0000    15.5000     0.0000  -199.9983  -449.0022    81.0000  1140.0007     1.0020    15.4190    17.0000   214.9970   545.000
      4  18000.407    104.000  38352.000  25262.000  13090.000 14618.0609  4444.9000     0.0000    44.0000    44.0000    15.5000     0.0000  -199.9983  -449.0022    81.0000  1140.0007     1.0020    15.4190    17.0000   214.9970   545.000
      5  18000.625    106.000  37927.000  25125.000  12802.000 14618.0609  4444.9000     0.0000    44.0000    44.0000    15.5000     0.0000  -199.9983  -449.0022    81.0000  1140.0007     1.0020    15.4190    17.0000   214.9970   545.000
      6  18001.000    111.000  37931.000  25219.000  12712.000 14618.0609  4444.9000     0.0000    44.0000    44.0000    15.5000     0.0000  -199.9983  -449.0022    81.0000  1140.0007     1.0020    15.4190    17.0000   214.9970   545.000
      7  18000.797    106.000  37949.000  25027.000  12922.000 14618.0609  4444.9000     0.0000    44.0000    44.0000    15.5000     0.0000  -199.9983  -449.0022    81.0000  1140.0007     1.0020    15.4190    17.0000   214.9970   545.000
      8  18000.953    108.000  37657.000  25022.000  12635.000 14618.0609  4444.9000     0.0000    44.0000    44.0000    15.5000     0.0000  -199.9983  -449.0022    81.0000  1140.0007     1.0020    15.4190    17.0000   214.9970   545.000
      9  18000.594    112.000  38201.000  25118.000  13083.000 14618.0609  4444.9000     0.0000    44.0000    44.0000    15.5000     0.0000  -199.9983  -449.0022    81.0000  1140.0007     1.0020    15.4190    17.0000   214.9970   545.000
     10  18000.828    123.000  37534.000  24924.000  12610.000 14618.0609  4444.9000     0.0000    44.0000    44.0000    15.5000     0.0000  -199.9983  -449.0022    81.0000  1140.0007     1.0020    15.4190    17.0000   214.9970   545.000
     11  18001.031    117.000  37271.000  24761.000  12510.000 14618.0609  4444.9000     0.0000    44.0000    44.0000    15.5000     0.0000  -199.9983  -449.0022    81.0000  1140.0007     1.0020    15.4190    17.0000   214.9970   545.000
# Footer Info = Add information here
# 6:13:14 AM  10/2/2017   scan completed.

12:15:13 PM  10/2/2017    Executing "method chiller set_setpoint d 25.000000"
                          Derived from "set_chiller 25"

Return Code: 0
Integer returned values:   
Double returned values:   25.000000

String returned values:   


1:46:23 PM  10/6/2017    Executing "let __active_table_scans.in_progress "0""

Setting variable "__active_table_scans.in_progress" (current value = "0.000000") to "0.000000".

Abort issued!!
#  galil_motor_controller_1:  "galil_progs_filename" not found in configuration file
No program file will be loaded.#  galil_motor_controller_10:  "galil_progs_filename" not found in configuration file
No program file will be loaded.#  galil_motor_controller_2:  "galil_progs_filename" not found in configuration file
No program file will be loaded.#  galil_motor_controller_3:  "galil_progs_filename" not found in configuration file
No program file will be loaded.#  galil_motor_controller_4:  "galil_progs_filename" not found in configuration file
No program file will be loaded.#  galil_motor_controller_5:  "galil_progs_filename" not found in configuration file
No program file will be loaded.
Motor consistancy check failed for hum_vert.
The previously recorded position was 16.99996.
The current position read from the controller is 16.99996.
****Motor [hum_vert] initialized to previosly recorded position [16.99996].
The following error messages were obtained while restoring the experiment status:

The specified default counting channel, , is not a valid counter channel.

The following error messages were obtained while restoring the experiment status:

The specified default counting channel, , is not a valid counter channel.


6:31:57 PM  10/6/2017    Executing "initialize"
                         Derived from "init"

Reinitializing experiment ... The following error messages were obtained while restoring the experiment status:

The specified default counting channel, , is not a valid counter channel.

 Completed initialization.


6:32:40 PM  10/6/2017    Executing "drive sdd 12"

Driving to the following position: ""

Destination Motor Positions:
motor           position
flange_det_dist 11.91900

Drive completed.


6:32:52 PM  10/6/2017    Executing "drive dcal 3"

Driving to the following position: ""

Destination Motor Positions:
motor           position
dcal            3.00000

Drive completed.


6:33:08 PM  10/6/2017    Executing "drive vs1 2000"

Driving to the following position: ""

Destination Motor Positions:
motor           position
selector_speed  2000.00000

Drive completed.


6:33:12 PM  10/6/2017    Executing "drive vs1 2000"

Driving to the following position: ""

Destination Motor Positions:
motor           position
selector_speed  2000.00000

Drive completed.


6:34:13 PM  10/6/2017    Executing "drive nguides 3"

Driving to the following position: ""

Destination Motor Positions:
motor           position
coll_1          guide
coll_2          guide
coll_3          guide
coll_4          aperture
coll_5          aperture
coll_6          aperture
coll_7          aperture

Drive completed.


6:34:39 PM  10/6/2017    Executing "drive nguides 3"

Driving to the following position: ""

Destination Motor Positions:
motor           position
coll_1          guide
coll_2          guide
coll_3          guide
coll_4          aperture
coll_5          aperture
coll_6          aperture
coll_7          aperture

Drive completed.


6:44:45 PM  10/6/2017    Executing "let __active_table_scans.in_progress "0""

Setting variable "__active_table_scans.in_progress" (current value = "") to "0.000000".

Abort issued!!
The following error messages were obtained while restoring the experiment status:

The specified default counting channel, , is not a valid counter channel.


5:38:37 PM  2/20/2019    Executing "comment "--------------------Begin Table Scans/Sample Scans Preamble""

COMMENT:
--------------------Begin Table Scans/Sample Scans Preamble


5:38:37 PM  2/20/2019    Executing "reset_active_scan_data"

Resetting active scan data.
5:38:39 PM  2/20/2019    Executing "scantitle """

Setting the scantitle to:



5:38:39 PM  2/20/2019    Executing "set_sample_info_sample_changer "Banjo" 15"

Setting sample info sample changer name to Banjo 
with 15 changer positions.

5:38:39 PM  2/20/2019    Executing "set_sample_info_instrument_config "SQ_6A_SDD15.5m_Banjo" "0.003-0.8""

Setting sample info instrument configuration name to SQ_6A_SDD15.5m_Banjo.
 
5:38:39 PM  2/20/2019    Executing "set_sample_info_parameter_config "No Parameters" "" """

Setting sample info parameter configuration name to No Parameters.
 
5:38:39 PM  2/20/2019    Executing "set_sample_info_setup_order "0.003-0.8""

Setting sample info setup order to "0.003-0.8".

5:38:39 PM  2/20/2019    Executing "set_sample_info_scan_order "Setup Order""

Setting sample info scan order to "Setup Order".
 
5:38:39 PM  2/20/2019    Executing "set_sample_info_do_transmission_scans "false""

Setting sample info do_transmission_scans to "false".

5:38:39 PM  2/20/2019    Executing "set_sample_info_specify_frames "false""

Setting sample info specify_frames to "false".
 
5:38:40 PM  2/20/2019    Executing "set_sample_info_background_columns_names """

Setting sample info background columns names to "".
 
5:38:40 PM  2/20/2019    Executing "set_sample_info_background_columns_default_values """

Setting sample info background columns default values to "".
 
5:38:40 PM  2/20/2019    Executing "set_sample_info_sample_columns_names """

Setting sample info sample columns names to "".
 
5:38:40 PM  2/20/2019    Executing "set_sample_info_sample_columns_default_values """

Setting sample info sample columns default values to "".
 
5:38:40 PM  2/20/2019    Executing "set_sample_info_sample_id 1 """

Setting sample info sample id to  
for changer position 1.

5:38:40 PM  2/20/2019    Executing "set_sample_info_sample_name 1 "dark no reactor""

Setting sample info sample name to dark no reactor 
for changer position 1.

5:38:40 PM  2/20/2019    Executing "set_sample_info_sample_thickness 1 "2.000000""

Setting sample info sample thickness to 2.000000 mm 
for changer position 1.

5:38:40 PM  2/20/2019    Executing "set_sample_info_sample_columns_values 1 ",""

Setting sample info sample columns values to "," 
for changer position 1.

5:38:40 PM  2/20/2019    Executing "set_sample_info_background_columns_values 1 """

Setting sample info background columns values to "" 
for changer position 1.

5:38:41 PM  2/20/2019    Executing "set_sample_info_sample_type 1 "Sample""

Setting sample info sample type to Sample 
for changer position 1.

5:38:41 PM  2/20/2019    Executing "set_sample_info_do_scan 1 "true""

Setting sample info do_scan value to true 
for changer position 1.

5:38:41 PM  2/20/2019    Executing "set_sample_info_scan_times 1 "2.000000""

Setting sample info scan times values to "2.000000" 
for changer position 1.

5:38:41 PM  2/20/2019    Executing "set_sample_info_frame_counts 1 "1""

Setting sample info frame counts values to "1" 
for changer position 1.

5:38:41 PM  2/20/2019    Executing "set_sample_info_parameter_columns_values 1 """

Setting sample info parameter columns values to "" 
for changer position 1.

5:38:41 PM  2/20/2019    Executing "set_sample_info_sample_id 2 """

Setting sample info sample id to  
for changer position 2.

5:38:41 PM  2/20/2019    Executing "set_sample_info_sample_name 2 "NJ2""

Setting sample info sample name to NJ2 
for changer position 2.

5:38:41 PM  2/20/2019    Executing "set_sample_info_sample_thickness 2 "2.000000""

Setting sample info sample thickness to 2.000000 mm 
for changer position 2.

5:38:41 PM  2/20/2019    Executing "set_sample_info_sample_columns_values 2 ",dkale""

Setting sample info sample columns values to ",dkale" 
for changer position 2.

5:38:41 PM  2/20/2019    Executing "set_sample_info_background_columns_values 2 """

Setting sample info background columns values to "" 
for changer position 2.

5:38:42 PM  2/20/2019    Executing "set_sample_info_sample_type 2 "Sample""

Setting sample info sample type to Sample 
for changer position 2.

5:38:42 PM  2/20/2019    Executing "set_sample_info_do_scan 2 "true""

Setting sample info do_scan value to true 
for changer position 2.

5:38:42 PM  2/20/2019    Executing "set_sample_info_scan_times 2 "2.000000""

Setting sample info scan times values to "2.000000" 
for changer position 2.

5:38:42 PM  2/20/2019    Executing "set_sample_info_frame_counts 2 "1""

Setting sample info frame counts values to "1" 
for changer position 2.

5:38:42 PM  2/20/2019    Executing "set_sample_info_parameter_columns_values 2 """

Setting sample info parameter columns values to "" 
for changer position 2.

5:38:42 PM  2/20/2019    Executing "set_sample_info_sample_id 3 """

Setting sample info sample id to  
for changer position 3.

5:38:42 PM  2/20/2019    Executing "set_sample_info_sample_name 3 "NJ3""

Setting sample info sample name to NJ3 
for changer position 3.

5:38:42 PM  2/20/2019    Executing "set_sample_info_sample_thickness 3 "2.000000""

Setting sample info sample thickness to 2.000000 mm 
for changer position 3.

5:38:42 PM  2/20/2019    Executing "set_sample_info_sample_columns_values 3 ",dkale""

Setting sample info sample columns values to ",dkale" 
for changer position 3.

5:38:42 PM  2/20/2019    Executing "set_sample_info_background_columns_values 3 """

Setting sample info background columns values to "" 
for changer position 3.

5:38:43 PM  2/20/2019    Executing "set_sample_info_sample_type 3 "Sample""

Setting sample info sample type to Sample 
for changer position 3.

5:38:43 PM  2/20/2019    Executing "set_sample_info_do_scan 3 "true""

Setting sample info do_scan value to true 
for changer position 3.

5:38:43 PM  2/20/2019    Executing "set_sample_info_scan_times 3 "2.000000""

Setting sample info scan times values to "2.000000" 
for changer position 3.

5:38:43 PM  2/20/2019    Executing "set_sample_info_frame_counts 3 "1""

Setting sample info frame counts values to "1" 
for changer position 3.

5:38:43 PM  2/20/2019    Executing "set_sample_info_parameter_columns_values 3 """

Setting sample info parameter columns values to "" 
for changer position 3.

5:38:44 PM  2/20/2019    Executing "set_sample_info_sample_id 4 """

Setting sample info sample id to  
for changer position 4.

5:38:44 PM  2/20/2019    Executing "set_sample_info_sample_name 4 "NJ4""

Setting sample info sample name to NJ4 
for changer position 4.

5:38:44 PM  2/20/2019    Executing "set_sample_info_sample_thickness 4 "2.000000""

Setting sample info sample thickness to 2.000000 mm 
for changer position 4.

5:38:44 PM  2/20/2019    Executing "set_sample_info_sample_columns_values 4 ",dkale""

Setting sample info sample columns values to ",dkale" 
for changer position 4.

5:38:44 PM  2/20/2019    Executing "set_sample_info_background_columns_values 4 """

Setting sample info background columns values to "" 
for changer position 4.

5:38:44 PM  2/20/2019    Executing "set_sample_info_sample_type 4 "Sample""

Setting sample info sample type to Sample 
for changer position 4.

5:38:44 PM  2/20/2019    Executing "set_sample_info_do_scan 4 "true""

Setting sample info do_scan value to true 
for changer position 4.

5:38:44 PM  2/20/2019    Executing "set_sample_info_scan_times 4 "2.000000""

Setting sample info scan times values to "2.000000" 
for changer position 4.

5:38:44 PM  2/20/2019    Executing "set_sample_info_frame_counts 4 "1""

Setting sample info frame counts values to "1" 
for changer position 4.

5:38:44 PM  2/20/2019    Executing "set_sample_info_parameter_columns_values 4 """

Setting sample info parameter columns values to "" 
for changer position 4.

5:38:44 PM  2/20/2019    Executing "set_sample_info_sample_id 5 """

Setting sample info sample id to  
for changer position 5.

5:38:45 PM  2/20/2019    Executing "set_sample_info_sample_name 5 """

Setting sample info sample name to  
for changer position 5.

5:38:45 PM  2/20/2019    Executing "set_sample_info_sample_thickness 5 "0.000000""

Setting sample info sample thickness to 0.000000 mm 
for changer position 5.

5:38:45 PM  2/20/2019    Executing "set_sample_info_sample_columns_values 5 """

Setting sample info sample columns values to "" 
for changer position 5.

5:38:45 PM  2/20/2019    Executing "set_sample_info_background_columns_values 5 """

Setting sample info background columns values to "" 
for changer position 5.

5:38:45 PM  2/20/2019    Executing "set_sample_info_sample_type 5 "Sample""

Setting sample info sample type to Sample 
for changer position 5.

5:38:45 PM  2/20/2019    Executing "set_sample_info_do_scan 5 "true""

Setting sample info do_scan value to true 
for changer position 5.

5:38:45 PM  2/20/2019    Executing "set_sample_info_scan_times 5 "2.000000""

Setting sample info scan times values to "2.000000" 
for changer position 5.

5:38:45 PM  2/20/2019    Executing "set_sample_info_frame_counts 5 "1""

Setting sample info frame counts values to "1" 
for changer position 5.

5:38:46 PM  2/20/2019    Executing "set_sample_info_parameter_columns_values 5 """

Setting sample info parameter columns values to "" 
for changer position 5.

5:38:46 PM  2/20/2019    Executing "set_sample_info_sample_id 6 """

Setting sample info sample id to  
for changer position 6.

5:38:46 PM  2/20/2019    Executing "set_sample_info_sample_name 6 """

Setting sample info sample name to  
for changer position 6.

5:38:46 PM  2/20/2019    Executing "set_sample_info_sample_thickness 6 "0.000000""

Setting sample info sample thickness to 0.000000 mm 
for changer position 6.

5:38:46 PM  2/20/2019    Executing "set_sample_info_sample_columns_values 6 """

Setting sample info sample columns values to "" 
for changer position 6.

5:38:46 PM  2/20/2019    Executing "set_sample_info_background_columns_values 6 """

Setting sample info background columns values to "" 
for changer position 6.

5:38:46 PM  2/20/2019    Executing "set_sample_info_sample_type 6 "Sample""

Setting sample info sample type to Sample 
for changer position 6.

5:38:46 PM  2/20/2019    Executing "set_sample_info_do_scan 6 "false""

Setting sample info do_scan value to false 
for changer position 6.

5:38:46 PM  2/20/2019    Executing "set_sample_info_scan_times 6 "20000.000000""

Setting sample info scan times values to "20000.000000" 
for changer position 6.

5:38:46 PM  2/20/2019    Executing "set_sample_info_frame_counts 6 "1""

Setting sample info frame counts values to "1" 
for changer position 6.

5:38:46 PM  2/20/2019    Executing "set_sample_info_parameter_columns_values 6 """

Setting sample info parameter columns values to "" 
for changer position 6.

5:38:47 PM  2/20/2019    Executing "set_sample_info_sample_id 7 """

Setting sample info sample id to  
for changer position 7.

5:38:47 PM  2/20/2019    Executing "set_sample_info_sample_name 7 """

Setting sample info sample name to  
for changer position 7.

5:38:47 PM  2/20/2019    Executing "set_sample_info_sample_thickness 7 "0.000000""

Setting sample info sample thickness to 0.000000 mm 
for changer position 7.

5:38:47 PM  2/20/2019    Executing "set_sample_info_sample_columns_values 7 """

Setting sample info sample columns values to "" 
for changer position 7.

5:38:47 PM  2/20/2019    Executing "set_sample_info_background_columns_values 7 """

Setting sample info background columns values to "" 
for changer position 7.

5:38:47 PM  2/20/2019    Executing "set_sample_info_sample_type 7 "Sample""

Setting sample info sample type to Sample 
for changer position 7.

5:38:47 PM  2/20/2019    Executing "set_sample_info_do_scan 7 "false""

Setting sample info do_scan value to false 
for changer position 7.

5:38:47 PM  2/20/2019    Executing "set_sample_info_scan_times 7 "20000.000000""

Setting sample info scan times values to "20000.000000" 
for changer position 7.

5:38:47 PM  2/20/2019    Executing "set_sample_info_frame_counts 7 "1""

Setting sample info frame counts values to "1" 
for changer position 7.

5:38:47 PM  2/20/2019    Executing "set_sample_info_parameter_columns_values 7 """

Setting sample info parameter columns values to "" 
for changer position 7.

5:38:48 PM  2/20/2019    Executing "set_sample_info_sample_id 8 """

Setting sample info sample id to  
for changer position 8.

5:38:48 PM  2/20/2019    Executing "set_sample_info_sample_name 8 """

Setting sample info sample name to  
for changer position 8.

5:38:48 PM  2/20/2019    Executing "set_sample_info_sample_thickness 8 "0.000000""

Setting sample info sample thickness to 0.000000 mm 
for changer position 8.

5:38:48 PM  2/20/2019    Executing "set_sample_info_sample_columns_values 8 """

Setting sample info sample columns values to "" 
for changer position 8.

5:38:48 PM  2/20/2019    Executing "set_sample_info_background_columns_values 8 """

Setting sample info background columns values to "" 
for changer position 8.

5:38:49 PM  2/20/2019    Executing "set_sample_info_sample_type 8 "Sample""

Setting sample info sample type to Sample 
for changer position 8.

5:38:49 PM  2/20/2019    Executing "set_sample_info_do_scan 8 "false""

Setting sample info do_scan value to false 
for changer position 8.

5:38:49 PM  2/20/2019    Executing "set_sample_info_scan_times 8 "20000.000000""

Setting sample info scan times values to "20000.000000" 
for changer position 8.

5:38:49 PM  2/20/2019    Executing "set_sample_info_frame_counts 8 "1""

Setting sample info frame counts values to "1" 
for changer position 8.

5:38:49 PM  2/20/2019    Executing "set_sample_info_parameter_columns_values 8 """

Setting sample info parameter columns values to "" 
for changer position 8.

5:38:49 PM  2/20/2019    Executing "set_sample_info_sample_id 9 """

Setting sample info sample id to  
for changer position 9.

5:38:49 PM  2/20/2019    Executing "set_sample_info_sample_name 9 """

Setting sample info sample name to  
for changer position 9.

5:38:49 PM  2/20/2019    Executing "set_sample_info_sample_thickness 9 "0.000000""

Setting sample info sample thickness to 0.000000 mm 
for changer position 9.

5:38:49 PM  2/20/2019    Executing "set_sample_info_sample_columns_values 9 """

Setting sample info sample columns values to "" 
for changer position 9.

5:38:49 PM  2/20/2019    Executing "set_sample_info_background_columns_values 9 """

Setting sample info background columns values to "" 
for changer position 9.

5:38:50 PM  2/20/2019    Executing "set_sample_info_sample_type 9 "Sample""

Setting sample info sample type to Sample 
for changer position 9.

5:38:50 PM  2/20/2019    Executing "set_sample_info_do_scan 9 "false""

Setting sample info do_scan value to false 
for changer position 9.

5:38:50 PM  2/20/2019    Executing "set_sample_info_scan_times 9 "20000.000000""

Setting sample info scan times values to "20000.000000" 
for changer position 9.

5:38:50 PM  2/20/2019    Executing "set_sample_info_frame_counts 9 "1""

Setting sample info frame counts values to "1" 
for changer position 9.

5:38:50 PM  2/20/2019    Executing "set_sample_info_parameter_columns_values 9 """

Setting sample info parameter columns values to "" 
for changer position 9.

5:38:50 PM  2/20/2019    Executing "set_sample_info_sample_id 10 """

Setting sample info sample id to  
for changer position 10.

5:38:50 PM  2/20/2019    Executing "set_sample_info_sample_name 10 """

Setting sample info sample name to  
for changer position 10.

5:38:50 PM  2/20/2019    Executing "set_sample_info_sample_thickness 10 "0.000000""

Setting sample info sample thickness to 0.000000 mm 
for changer position 10.

5:38:50 PM  2/20/2019    Executing "set_sample_info_sample_columns_values 10 """

Setting sample info sample columns values to "" 
for changer position 10.

5:38:50 PM  2/20/2019    Executing "set_sample_info_background_columns_values 10 """

Setting sample info background columns values to "" 
for changer position 10.

5:38:50 PM  2/20/2019    Executing "set_sample_info_sample_type 10 "Sample""

Setting sample info sample type to Sample 
for changer position 10.

5:38:51 PM  2/20/2019    Executing "set_sample_info_do_scan 10 "false""

Setting sample info do_scan value to false 
for changer position 10.

5:38:51 PM  2/20/2019    Executing "set_sample_info_scan_times 10 "20000.000000""

Setting sample info scan times values to "20000.000000" 
for changer position 10.

5:38:51 PM  2/20/2019    Executing "set_sample_info_frame_counts 10 "1""

Setting sample info frame counts values to "1" 
for changer position 10.

5:38:51 PM  2/20/2019    Executing "set_sample_info_parameter_columns_values 10 """

Setting sample info parameter columns values to "" 
for changer position 10.

5:38:51 PM  2/20/2019    Executing "set_sample_info_sample_id 11 """

Setting sample info sample id to  
for changer position 11.

5:38:51 PM  2/20/2019    Executing "set_sample_info_sample_name 11 """

Setting sample info sample name to  
for changer position 11.

5:38:51 PM  2/20/2019    Executing "set_sample_info_sample_thickness 11 "0.000000""

Setting sample info sample thickness to 0.000000 mm 
for changer position 11.

5:38:51 PM  2/20/2019    Executing "set_sample_info_sample_columns_values 11 """

Setting sample info sample columns values to "" 
for changer position 11.

5:38:51 PM  2/20/2019    Executing "set_sample_info_background_columns_values 11 """

Setting sample info background columns values to "" 
for changer position 11.

5:38:51 PM  2/20/2019    Executing "set_sample_info_sample_type 11 "Sample""

Setting sample info sample type to Sample 
for changer position 11.

5:38:52 PM  2/20/2019    Executing "set_sample_info_do_scan 11 "false""

Setting sample info do_scan value to false 
for changer position 11.

5:38:52 PM  2/20/2019    Executing "set_sample_info_scan_times 11 "20000.000000""

Setting sample info scan times values to "20000.000000" 
for changer position 11.

5:38:52 PM  2/20/2019    Executing "set_sample_info_frame_counts 11 "1""

Setting sample info frame counts values to "1" 
for changer position 11.

5:38:52 PM  2/20/2019    Executing "set_sample_info_parameter_columns_values 11 """

Setting sample info parameter columns values to "" 
for changer position 11.

5:38:52 PM  2/20/2019    Executing "set_sample_info_sample_id 12 """

Setting sample info sample id to  
for changer position 12.

5:38:52 PM  2/20/2019    Executing "set_sample_info_sample_name 12 """

Setting sample info sample name to  
for changer position 12.

5:38:52 PM  2/20/2019    Executing "set_sample_info_sample_thickness 12 "0.000000""

Setting sample info sample thickness to 0.000000 mm 
for changer position 12.

5:38:52 PM  2/20/2019    Executing "set_sample_info_sample_columns_values 12 """

Setting sample info sample columns values to "" 
for changer position 12.

5:38:52 PM  2/20/2019    Executing "set_sample_info_background_columns_values 12 """

Setting sample info background columns values to "" 
for changer position 12.

5:38:52 PM  2/20/2019    Executing "set_sample_info_sample_type 12 "Sample""

Setting sample info sample type to Sample 
for changer position 12.

5:38:53 PM  2/20/2019    Executing "set_sample_info_do_scan 12 "false""

Setting sample info do_scan value to false 
for changer position 12.

5:38:53 PM  2/20/2019    Executing "set_sample_info_scan_times 12 "20000.000000""

Setting sample info scan times values to "20000.000000" 
for changer position 12.

5:38:53 PM  2/20/2019    Executing "set_sample_info_frame_counts 12 "1""

Setting sample info frame counts values to "1" 
for changer position 12.

5:38:53 PM  2/20/2019    Executing "set_sample_info_parameter_columns_values 12 """

Setting sample info parameter columns values to "" 
for changer position 12.

5:38:53 PM  2/20/2019    Executing "set_sample_info_sample_id 13 """

Setting sample info sample id to  
for changer position 13.

5:38:54 PM  2/20/2019    Executing "set_sample_info_sample_name 13 """

Setting sample info sample name to  
for changer position 13.

5:38:54 PM  2/20/2019    Executing "set_sample_info_sample_thickness 13 "0.000000""

Setting sample info sample thickness to 0.000000 mm 
for changer position 13.

5:38:54 PM  2/20/2019    Executing "set_sample_info_sample_columns_values 13 """

Setting sample info sample columns values to "" 
for changer position 13.

5:38:54 PM  2/20/2019    Executing "set_sample_info_background_columns_values 13 """

Setting sample info background columns values to "" 
for changer position 13.

5:38:54 PM  2/20/2019    Executing "set_sample_info_sample_type 13 "Sample""

Setting sample info sample type to Sample 
for changer position 13.

5:38:54 PM  2/20/2019    Executing "set_sample_info_do_scan 13 "false""

Setting sample info do_scan value to false 
for changer position 13.

5:38:54 PM  2/20/2019    Executing "set_sample_info_scan_times 13 "20000.000000""

Setting sample info scan times values to "20000.000000" 
for changer position 13.

5:38:54 PM  2/20/2019    Executing "set_sample_info_frame_counts 13 "1""

Setting sample info frame counts values to "1" 
for changer position 13.

5:38:54 PM  2/20/2019    Executing "set_sample_info_parameter_columns_values 13 """

Setting sample info parameter columns values to "" 
for changer position 13.

5:38:54 PM  2/20/2019    Executing "set_sample_info_sample_id 14 """

Setting sample info sample id to  
for changer position 14.

5:38:54 PM  2/20/2019    Executing "set_sample_info_sample_name 14 """

Setting sample info sample name to  
for changer position 14.

5:38:55 PM  2/20/2019    Executing "set_sample_info_sample_thickness 14 "0.000000""

Setting sample info sample thickness to 0.000000 mm 
for changer position 14.

5:38:55 PM  2/20/2019    Executing "set_sample_info_sample_columns_values 14 """

Setting sample info sample columns values to "" 
for changer position 14.

5:38:55 PM  2/20/2019    Executing "set_sample_info_background_columns_values 14 """

Setting sample info background columns values to "" 
for changer position 14.

5:38:55 PM  2/20/2019    Executing "set_sample_info_sample_type 14 "Sample""

Setting sample info sample type to Sample 
for changer position 14.

5:38:55 PM  2/20/2019    Executing "set_sample_info_do_scan 14 "false""

Setting sample info do_scan value to false 
for changer position 14.

5:38:55 PM  2/20/2019    Executing "set_sample_info_scan_times 14 "20000.000000""

Setting sample info scan times values to "20000.000000" 
for changer position 14.

5:38:55 PM  2/20/2019    Executing "set_sample_info_frame_counts 14 "1""

Setting sample info frame counts values to "1" 
for changer position 14.

5:38:55 PM  2/20/2019    Executing "set_sample_info_parameter_columns_values 14 """

Setting sample info parameter columns values to "" 
for changer position 14.

5:38:55 PM  2/20/2019    Executing "set_sample_info_sample_id 15 """

Setting sample info sample id to  
for changer position 15.

5:38:55 PM  2/20/2019    Executing "set_sample_info_sample_name 15 """

Setting sample info sample name to  
for changer position 15.

5:38:56 PM  2/20/2019    Executing "set_sample_info_sample_thickness 15 "0.000000""

Setting sample info sample thickness to 0.000000 mm 
for changer position 15.

5:38:56 PM  2/20/2019    Executing "set_sample_info_sample_columns_values 15 """

Setting sample info sample columns values to "" 
for changer position 15.

5:38:56 PM  2/20/2019    Executing "set_sample_info_background_columns_values 15 """

Setting sample info background columns values to "" 
for changer position 15.

5:38:56 PM  2/20/2019    Executing "set_sample_info_sample_type 15 "Sample""

Setting sample info sample type to Sample 
for changer position 15.

5:38:56 PM  2/20/2019    Executing "set_sample_info_do_scan 15 "false""

Setting sample info do_scan value to false 
for changer position 15.

5:38:56 PM  2/20/2019    Executing "set_sample_info_scan_times 15 "20000.000000""

Setting sample info scan times values to "20000.000000" 
for changer position 15.

5:38:56 PM  2/20/2019    Executing "set_sample_info_frame_counts 15 "1""

Setting sample info frame counts values to "1" 
for changer position 15.

5:38:56 PM  2/20/2019    Executing "set_sample_info_parameter_columns_values 15 """

Setting sample info parameter columns values to "" 
for changer position 15.

5:38:56 PM  2/20/2019    Executing "use_sample_changer "Banjo""

Setting active sample changer to Banjo.

5:38:56 PM  2/20/2019    Executing "use_instrument_config "SQ_6A_SDD15.5m_Banjo""

Setting active instrument config to SQ_6A_SDD15.5m_Banjo.

5:38:57 PM  2/20/2019    Executing "use_parameter_config "No Parameters""

Setting active parameter config to No Parameters.

5:38:57 PM  2/20/2019    Executing "comment "--------------------End Table Scans/Sample Scans Preamble""

COMMENT:
--------------------End Table Scans/Sample Scans Preamble


5:38:57 PM  2/20/2019    Executing "reset_active_table_scans"

Resetting active table scan command info.
5:38:57 PM  2/20/2019    Executing "set_table_scan_command_info "do_table_scan 1 \220.003-0.8\22 \22Both\22 1" 1 "dark no reactor" "0.003-0.8" "Both" 2.000000 1 2.000000"

Setting  info for next table scan command.

5:38:57 PM  2/20/2019    Executing "set_table_scan_command_info "do_table_scan 2 \220.003-0.8\22 \22Both\22 2" 2 "NJ2" "0.003-0.8" "Both" 2.000000 1 2.000000"

Setting  info for next table scan command.

5:38:58 PM  2/20/2019    Executing "set_table_scan_command_info "do_table_scan 3 \220.003-0.8\22 \22Both\22 3" 3 "NJ3" "0.003-0.8" "Both" 2.000000 1 2.000000"

Setting  info for next table scan command.

5:38:58 PM  2/20/2019    Executing "set_table_scan_command_info "do_table_scan 4 \220.003-0.8\22 \22Both\22 4" 4 "NJ4" "0.003-0.8" "Both" 2.000000 1 2.000000"

Setting  info for next table scan command.

5:38:58 PM  2/20/2019    Executing "set_table_scan_command_info "do_table_scan 5 \220.003-0.8\22 \22Both\22 5" 5 "" "0.003-0.8" "Both" 2.000000 1 2.000000"

Setting  info for next table scan command.

5:38:58 PM  2/20/2019    Executing "let __active_table_scans.in_progress "1""

Setting variable "__active_table_scans.in_progress" (current value = "0") to "1.000000".

5:38:59 PM  2/20/2019    Executing "do_table_scan 1 "0.003-0.8" "Both" 1"


5:38:59 PM  2/20/2019    Executing "table_scan_initialize 1"

Initializing info for next table scan command.

5:38:59 PM  2/20/2019    Executing "do_table_scan 1 "0.003-0.8" "Both""


5:38:59 PM  2/20/2019    Executing "use_changer_pos 1"

Setting active sample changer position to 1 (valid sample info found).

5:38:59 PM  2/20/2019    Executing "use_setup "0.003-0.8" "Both""

Setting active setup to 0.003-0.8 and scan type to Both.

5:39:00 PM  2/20/2019    Executing "set_table_scan_title"

Automatically generating
scan title for table scan to:
dark no reactor(IC: SQ_6A_SDD15.5m_Banjo  S: 0.003-0.8  P:[])


5:39:00 PM  2/20/2019    Executing "do_parameters_start"


5:39:00 PM  2/20/2019    Executing "go_changer_pos"


5:39:00 PM  2/20/2019    Executing "drive sample_x 136.200000"

Driving to the following position: ""

Destination Motor Positions:
motor           position
sample_x        136.20000

Drive completed.


5:39:00 PM  2/20/2019    Executing "go_setup"


5:39:00 PM  2/20/2019    Executing "go_setup_beam_trap_in"


5:39:01 PM  2/20/2019    Executing "drive beam_trap_x 81.000000 trap_y_25mm 545.000000 aperture_x -89.700000 sdd 15.500000 det_west_wing_rot 1.400000 detector_trans 5.000000 lambda 6.000000"

Driving to the following position: ""

Destination Motor Positions:
motor           position
beam_trap_x     81.00000
trap_y_25mm     545.00000
aperture_x      -89.70000
det_west_wing_rot 1.40000
detector_trans  5.00000
flange_det_dist 15.42900
selector_speed  4444.87021

Drive completed.


5:39:01 PM  2/20/2019    Executing "if @(hv)<0.5 drive hv 1"


5:39:02 PM  2/20/2019    Executing "drive hv 1"

Driving to the following position: ""

Destination Motor Positions:
motor           position
highvoltagecmd  1.00000

[5:39:02 PM  2/20/2019]     ### Supplemental drive will be attempted for motor highvoltagecmd which has a current position of 2.489431.
Drive completed.


5:39:02 PM  2/20/2019    Executing "do_parameters_finish"


5:39:02 PM  2/20/2019    Executing "go_attenuator"


5:39:02 PM  2/20/2019    Executing "drive attenuator_pos open"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -449.00000

Drive completed.


5:39:03 PM  2/20/2019    Executing "table_scan_counting_initialize"

Initializing counting for current table scan command.

5:39:03 PM  2/20/2019    Executing "scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)"


# scan = 3
# date = 2/20/2019
# time = 5:39:03 PM
# experiment = Long Outage MP
# experiment_number = 456
# ipts_number = 17241
# cycle_number = 475
# command = scan n=@(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# builtin_command = scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# users = Shuo Qian
# local_contact = Shuo Qian
# scan_title = dark no reactor(IC: SQ_6A_SDD15.5m_Banjo  S: 0.003-0.8  P:[])
# samplename = dark no reactor
# sampletype = Sample
# preset_type = normal 
# preset_channel = time
# preset_value = 2.000000
# def_x = Pt.
# def_y = 
# col_headers = 
#   Pt.       time    monitor   detector detector_body detector_wing selector_speed selector_tilt        sdd    nguides aperture_x attenuator_pos beam_trap_x       dcal det_west_wing_rot flange_det_dist   sample_x trap_y_25mm
      1      2.748    508.000   2260.000   1668.000    592.000  4444.6395     0.0000    15.4990     0.0000   -89.7321  -448.9685    80.9979     2.9987     1.3966    15.4280   136.1557   545.003
# Footer Info = Add information here
# 5:39:09 PM  2/20/2019   scan completed.

5:39:09 PM  2/20/2019    Executing "table_scan_counting_finalize"

Finalizing counting for current table scan command.

5:39:09 PM  2/20/2019    Executing "go_attenuator_non_open"


5:39:09 PM  2/20/2019    Executing "drive attenuator_pos x3"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -384.00000

Drive completed.


5:39:09 PM  2/20/2019    Executing "reset_active_changer_pos_data"

Resetting active changer position data.
5:39:09 PM  2/20/2019    Executing "table_scan_finalize 1"

Finalizing info for next table scan command.

5:39:09 PM  2/20/2019    Executing "do_table_scan 2 "0.003-0.8" "Both" 2"


5:39:10 PM  2/20/2019    Executing "table_scan_initialize 2"

Initializing info for next table scan command.

5:39:10 PM  2/20/2019    Executing "do_table_scan 2 "0.003-0.8" "Both""


5:39:10 PM  2/20/2019    Executing "use_changer_pos 2"

Setting active sample changer position to 2 (valid sample info found).

5:39:10 PM  2/20/2019    Executing "use_setup "0.003-0.8" "Both""

Setting active setup to 0.003-0.8 and scan type to Both.

5:39:12 PM  2/20/2019    Executing "set_table_scan_title"

Automatically generating
scan title for table scan to:
NJ2(IC: SQ_6A_SDD15.5m_Banjo  S: 0.003-0.8  P:[])


5:39:12 PM  2/20/2019    Executing "do_parameters_start"


5:39:12 PM  2/20/2019    Executing "go_changer_pos"


5:39:12 PM  2/20/2019    Executing "drive sample_x 109.100000"

Driving to the following position: ""

Destination Motor Positions:
motor           position
sample_x        109.10000

Drive completed.


5:39:13 PM  2/20/2019    Executing "go_setup"


5:39:13 PM  2/20/2019    Executing "go_setup_beam_trap_in"


5:39:13 PM  2/20/2019    Executing "drive attenuator_pos x3"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -384.00000

Drive completed.


5:39:13 PM  2/20/2019    Executing "if @(hv)<0.5 drive hv 1"


5:39:14 PM  2/20/2019    Executing "do_parameters_finish"


5:39:14 PM  2/20/2019    Executing "go_attenuator"


5:39:14 PM  2/20/2019    Executing "drive attenuator_pos open"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -449.00000

Drive completed.


5:39:14 PM  2/20/2019    Executing "table_scan_counting_initialize"

Initializing counting for current table scan command.

5:39:14 PM  2/20/2019    Executing "scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)"


# scan = 4
# date = 2/20/2019
# time = 5:39:14 PM
# experiment = Long Outage MP
# experiment_number = 456
# ipts_number = 17241
# cycle_number = 475
# command = scan n=@(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# builtin_command = scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# users = Shuo Qian
# local_contact = Shuo Qian
# scan_title = NJ2(IC: SQ_6A_SDD15.5m_Banjo  S: 0.003-0.8  P:[])
# samplename = NJ2
# sampletype = Sample
# preset_type = normal 
# preset_channel = time
# preset_value = 2.000000
# def_x = Pt.
# def_y = 
# col_headers = 
#   Pt.       time    monitor   detector detector_body detector_wing selector_speed selector_tilt        sdd    nguides aperture_x attenuator_pos beam_trap_x       dcal det_west_wing_rot flange_det_dist   sample_x trap_y_25mm
      1      2.461    500.000      0.000      0.000      0.000  4444.6395     0.0000    15.4990     0.0000   -89.7321  -448.9897    80.9979     2.9987     1.3966    15.4280   109.1020   545.003
# Footer Info = Add information here
# 5:39:17 PM  2/20/2019   scan completed.

5:39:17 PM  2/20/2019    Executing "table_scan_counting_finalize"

Finalizing counting for current table scan command.

5:39:17 PM  2/20/2019    Executing "go_attenuator_non_open"


5:39:17 PM  2/20/2019    Executing "drive attenuator_pos x3"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -384.00000

Drive completed.


5:39:18 PM  2/20/2019    Executing "reset_active_changer_pos_data"

Resetting active changer position data.
5:39:18 PM  2/20/2019    Executing "table_scan_finalize 2"

Finalizing info for next table scan command.

5:39:18 PM  2/20/2019    Executing "do_table_scan 3 "0.003-0.8" "Both" 3"


5:39:19 PM  2/20/2019    Executing "table_scan_initialize 3"

Initializing info for next table scan command.

5:39:19 PM  2/20/2019    Executing "do_table_scan 3 "0.003-0.8" "Both""


5:39:19 PM  2/20/2019    Executing "use_changer_pos 3"

Setting active sample changer position to 3 (valid sample info found).

5:39:19 PM  2/20/2019    Executing "use_setup "0.003-0.8" "Both""

Setting active setup to 0.003-0.8 and scan type to Both.

5:39:21 PM  2/20/2019    Executing "set_table_scan_title"

Automatically generating
scan title for table scan to:
NJ3(IC: SQ_6A_SDD15.5m_Banjo  S: 0.003-0.8  P:[])


5:39:21 PM  2/20/2019    Executing "do_parameters_start"


5:39:21 PM  2/20/2019    Executing "go_changer_pos"


5:39:21 PM  2/20/2019    Executing "drive sample_x 82.000000"

Driving to the following position: ""

Destination Motor Positions:
motor           position
sample_x        82.00000

Drive completed.


5:39:21 PM  2/20/2019    Executing "go_setup"


5:39:21 PM  2/20/2019    Executing "go_setup_beam_trap_in"


5:39:22 PM  2/20/2019    Executing "drive attenuator_pos x3"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -384.00000

Drive completed.


5:39:22 PM  2/20/2019    Executing "if @(hv)<0.5 drive hv 1"


5:39:22 PM  2/20/2019    Executing "do_parameters_finish"


5:39:22 PM  2/20/2019    Executing "go_attenuator"


5:39:22 PM  2/20/2019    Executing "drive attenuator_pos open"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -449.00000

Drive completed.


5:39:23 PM  2/20/2019    Executing "table_scan_counting_initialize"

Initializing counting for current table scan command.

5:39:23 PM  2/20/2019    Executing "scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)"


# scan = 5
# date = 2/20/2019
# time = 5:39:23 PM
# experiment = Long Outage MP
# experiment_number = 456
# ipts_number = 17241
# cycle_number = 475
# command = scan n=@(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# builtin_command = scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# users = Shuo Qian
# local_contact = Shuo Qian
# scan_title = NJ3(IC: SQ_6A_SDD15.5m_Banjo  S: 0.003-0.8  P:[])
# samplename = NJ3
# sampletype = Sample
# preset_type = normal 
# preset_channel = time
# preset_value = 2.000000
# def_x = Pt.
# def_y = 
# col_headers = 
#   Pt.       time    monitor   detector detector_body detector_wing selector_speed selector_tilt        sdd    nguides aperture_x attenuator_pos beam_trap_x       dcal det_west_wing_rot flange_det_dist   sample_x trap_y_25mm
      1      2.504    491.000   3787.000   2781.000   1006.000  4444.6395     0.0000    15.4990     0.0000   -89.7321  -448.9839    80.9979     2.9987     1.3966    15.4280    81.9831   545.003
# Footer Info = Add information here
# 5:39:29 PM  2/20/2019   scan completed.

5:39:29 PM  2/20/2019    Executing "table_scan_counting_finalize"

Finalizing counting for current table scan command.

5:39:29 PM  2/20/2019    Executing "go_attenuator_non_open"


5:39:29 PM  2/20/2019    Executing "drive attenuator_pos x3"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -384.00000

Drive completed.


5:39:29 PM  2/20/2019    Executing "reset_active_changer_pos_data"

Resetting active changer position data.
5:39:29 PM  2/20/2019    Executing "table_scan_finalize 3"

Finalizing info for next table scan command.

5:39:29 PM  2/20/2019    Executing "do_table_scan 4 "0.003-0.8" "Both" 4"


5:39:30 PM  2/20/2019    Executing "table_scan_initialize 4"

Initializing info for next table scan command.

5:39:30 PM  2/20/2019    Executing "do_table_scan 4 "0.003-0.8" "Both""


5:39:30 PM  2/20/2019    Executing "use_changer_pos 4"

Setting active sample changer position to 4 (valid sample info found).

5:39:30 PM  2/20/2019    Executing "use_setup "0.003-0.8" "Both""

Setting active setup to 0.003-0.8 and scan type to Both.

5:39:32 PM  2/20/2019    Executing "set_table_scan_title"

Automatically generating
scan title for table scan to:
NJ4(IC: SQ_6A_SDD15.5m_Banjo  S: 0.003-0.8  P:[])


5:39:32 PM  2/20/2019    Executing "do_parameters_start"


5:39:32 PM  2/20/2019    Executing "go_changer_pos"


5:39:32 PM  2/20/2019    Executing "drive sample_x 54.900000"

Driving to the following position: ""

Destination Motor Positions:
motor           position
sample_x        54.90000

Drive completed.


5:39:33 PM  2/20/2019    Executing "go_setup"


5:39:33 PM  2/20/2019    Executing "go_setup_beam_trap_in"


5:39:33 PM  2/20/2019    Executing "if @(hv)<0.5 drive hv 1"


5:39:33 PM  2/20/2019    Executing "do_parameters_finish"


5:39:33 PM  2/20/2019    Executing "go_attenuator"


5:39:34 PM  2/20/2019    Executing "drive attenuator_pos open"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -449.00000

Drive completed.


5:39:34 PM  2/20/2019    Executing "table_scan_counting_initialize"

Initializing counting for current table scan command.

5:39:34 PM  2/20/2019    Executing "scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)"


# scan = 6
# date = 2/20/2019
# time = 5:39:34 PM
# experiment = Long Outage MP
# experiment_number = 456
# ipts_number = 17241
# cycle_number = 475
# command = scan n=@(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# builtin_command = scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# users = Shuo Qian
# local_contact = Shuo Qian
# scan_title = NJ4(IC: SQ_6A_SDD15.5m_Banjo  S: 0.003-0.8  P:[])
# samplename = NJ4
# sampletype = Sample
# preset_type = normal 
# preset_channel = time
# preset_value = 2.000000
# def_x = Pt.
# def_y = 
# col_headers = 
#   Pt.       time    monitor   detector detector_body detector_wing selector_speed selector_tilt        sdd    nguides aperture_x attenuator_pos beam_trap_x       dcal det_west_wing_rot flange_det_dist   sample_x trap_y_25mm
      1      2.453    510.000   2225.000   1636.000    589.000  4444.6395     0.0000    15.4990     0.0000   -89.7321  -449.0128    80.9979     2.9987     1.3966    15.4280    54.9258   545.003
# Footer Info = Add information here
# 5:39:39 PM  2/20/2019   scan completed.

5:39:39 PM  2/20/2019    Executing "table_scan_counting_finalize"

Finalizing counting for current table scan command.

5:39:39 PM  2/20/2019    Executing "go_attenuator_non_open"


5:39:39 PM  2/20/2019    Executing "drive attenuator_pos x3"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -384.00000

Drive completed.


5:39:40 PM  2/20/2019    Executing "reset_active_changer_pos_data"

Resetting active changer position data.
5:39:40 PM  2/20/2019    Executing "table_scan_finalize 4"

Finalizing info for next table scan command.

5:39:40 PM  2/20/2019    Executing "do_table_scan 5 "0.003-0.8" "Both" 5"


5:39:40 PM  2/20/2019    Executing "table_scan_initialize 5"

Initializing info for next table scan command.

5:39:40 PM  2/20/2019    Executing "do_table_scan 5 "0.003-0.8" "Both""


5:39:40 PM  2/20/2019    Executing "use_changer_pos 5"

Setting active sample changer position to 5 (valid sample info found).

5:39:40 PM  2/20/2019    Executing "use_setup "0.003-0.8" "Both""

Setting active setup to 0.003-0.8 and scan type to Both.

5:39:42 PM  2/20/2019    Executing "set_table_scan_title"

Automatically generating
scan title for table scan to:
(IC: SQ_6A_SDD15.5m_Banjo  S: 0.003-0.8  P:[])


5:39:42 PM  2/20/2019    Executing "do_parameters_start"


5:39:43 PM  2/20/2019    Executing "go_changer_pos"


5:39:43 PM  2/20/2019    Executing "drive sample_x 27.800000"

Driving to the following position: ""

Destination Motor Positions:
motor           position
sample_x        27.80000

Drive completed.


5:39:43 PM  2/20/2019    Executing "go_setup"


5:39:44 PM  2/20/2019    Executing "go_setup_beam_trap_in"


5:39:44 PM  2/20/2019    Executing "drive attenuator_pos x3"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -384.00000

Drive completed.


5:39:44 PM  2/20/2019    Executing "if @(hv)<0.5 drive hv 1"


5:39:44 PM  2/20/2019    Executing "do_parameters_finish"


5:39:44 PM  2/20/2019    Executing "go_attenuator"


5:39:44 PM  2/20/2019    Executing "drive attenuator_pos open"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -449.00000

Drive completed.


5:39:45 PM  2/20/2019    Executing "table_scan_counting_initialize"

Initializing counting for current table scan command.

5:39:45 PM  2/20/2019    Executing "scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)"


# scan = 7
# date = 2/20/2019
# time = 5:39:45 PM
# experiment = Long Outage MP
# experiment_number = 456
# ipts_number = 17241
# cycle_number = 475
# command = scan n=@(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# builtin_command = scan n @(__active_setup.frame_count)-1 preset time @(__active_setup.scan_time)
# users = Shuo Qian
# local_contact = Shuo Qian
# scan_title = (IC: SQ_6A_SDD15.5m_Banjo  S: 0.003-0.8  P:[])
# samplename = 
# sampletype = Sample
# preset_type = normal 
# preset_channel = time
# preset_value = 2.000000
# def_x = Pt.
# def_y = 
# col_headers = 
#   Pt.       time    monitor   detector detector_body detector_wing selector_speed selector_tilt        sdd    nguides aperture_x attenuator_pos beam_trap_x       dcal det_west_wing_rot flange_det_dist   sample_x trap_y_25mm
      1      2.441    542.000   2256.000   1676.000    580.000  4444.6395     0.0000    15.4990     0.0000   -89.7321  -448.9717    80.9979     2.9987     1.3966    15.4280    27.7939   545.003
# Footer Info = Add information here
# 5:39:49 PM  2/20/2019   scan completed.

5:39:49 PM  2/20/2019    Executing "table_scan_counting_finalize"

Finalizing counting for current table scan command.

5:39:49 PM  2/20/2019    Executing "go_attenuator_non_open"


5:39:49 PM  2/20/2019    Executing "drive attenuator_pos x3"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -384.00000

Drive completed.


5:39:49 PM  2/20/2019    Executing "reset_active_changer_pos_data"

Resetting active changer position data.
5:39:49 PM  2/20/2019    Executing "table_scan_finalize 5"

Finalizing info for next table scan command.

5:39:49 PM  2/20/2019    Executing "drive attenuator_pos close"
                         Derived from "attclose"

Driving to the following position: ""

Destination Motor Positions:
motor           position
attenuator_pos  -7.00000

Drive completed.


5:39:50 PM  2/20/2019    Executing "go_changer_park"


5:39:50 PM  2/20/2019    Executing "drive sample_x 215.000000"

Driving to the following position: ""

Destination Motor Positions:
motor           position
sample_x        215.00000

Drive completed.


5:39:50 PM  2/20/2019    Executing "let __active_table_scans.in_progress "0""

Setting variable "__active_table_scans.in_progress" (current value = "1.000000") to "0.000000".

5:40:16 PM  2/20/2019    Executing "let __active_table_scans.in_progress "0""

